# ew2ringserver Configuration File

(last revised April 22, 2015)

    #
    #  ew2ringserver configuration file
    #
    #
     MyModuleId     MOD_EW2RINGSERVER   # module id for this program
     RingName       WAVE_RING           # transport ring to use for input
     RSAddress      localhost:16000     # address of destination ringserver
                                        # in host:port format
     HeartBeatInt   30                  # EW internal heartbeat interval (sec)
     LogFile        1                   # If 0, don't write logfile; if 1, do
                                        # if 2, write to module log but not to
                                        # stderr/stdout
    #
    # Logos of messages to export to client systems
    #              Installation       Module       Message Type
     GetMsgLogo    INST_WILDCARD   MOD_WILDCARD    TYPE_TRACEBUF2
    #GetMsgLogo    INST_WILDCARD   MOD_WILDCARD    TYPE_MSEED
    # For TYPE_MSEED the miniSEED message must be 512-byte records, otherwise ignored.

     MaxMsgSize     4096          # maximum size (bytes) for input/output msgs
     QueueSize	1000          # max# messages in internal circular msg buffer

    #
    # Optional parameters
    #
    #Verbosity  0                 # set verbosity, useful for diagnostics
    #FlushLatency 300             # flush any buffered data streams idle for this many seconds
    #ReconnectInterval 10         # reconnect to ringserver at this interval in seconds
    #Int32Encoding STEIM2         # specify miniSEED encoding for 32-bit integers, default STEIM2
                                  #   possible values are STEIM2, STEIM1 or INT32 (no compression)

    # List of station/channel/network/loc codes to process.
    #--------------------------------------------------------
    #
    # Use any combination of Send_scnl (to send data as-is) and
    #   Send_scnl_remap (to change the SCNL on the fly) commands.
    # Use * as a wildcard for any field. A wildcard in the
    #   "map to" fields of Send_scnl_remap means that field will
    #   not be renamed.
    #
    #                  send SCNL     map to SCNL
    # Send_scnl       JMP ASZ NC 01                # send this specific channel
    # Send_scnl       JPS *   NC *                 # send all components of JPS NC
    # Send_scnl_remap JGR VHZ NC --   *   EHZ * *  # change component code only
    # Send_scnl_remap CAL *   NC *    ALM *   * *  # send all component of CAL, but
                                                   # change the station code to ALM
    Send_scnl * * * *

Module Index | ew2ringserver Overview