# Coda AAV Configuration File Commands

(last revised 25 October 2012)

    #
    #  coda_aav's Configuration File
    #
    MyModId       MOD_CODA_AAV     # This instance of pick_ew
    StaFile       "pick_ew.sta"    # File containing station name/pin# info
    InRing           WAVE_RING     # Transport ring to find waveform data on,
    OutRing          PICK_RING     # Transport ring to write output to,
    HeartbeatInt            30     # Heartbeat interval, in seconds,
    Debug                    0     # If 1, print debugging message

    # Specify which messages to look at with Getlogo commands.
    #   GetLogo
    # The message_type must be either TYPE_TRACEBUF or TYPE_TRACEBUF2.
    # Use as many GetLogo commands as you need.
    # If no GetLogo commands are given, pick_ew will look at all
    # TYPE_TRACEBUF and TYPE_TRACEBUF2 messages in InRing.
    #-----------------------------------------------------------------
    GetLogo  INST_WILDCARD  MOD_WILDCARD  TYPE_TRACEBUF2

Module Index | Coda AAV Overview