#
Ewdrift Configuration File

(last revised 9 February, 2012)

    #
    #                     Configuration File for Ewdrift
    #
     MyModId            MOD_DRIFT
     InRing             WAVE_RING # Transport ring to find waveform data on,
     OutRing            DRIFT_RING # Transport ring to write output to,
                                  # InRing and OutRing may be the same.
     HeartBeatInterval  30        # Heartbeat interval, in seconds,
     LogFile            1         # 1 -> Keep log file, 0 -> no log file
                                  # 2 -> log to file but not to stderr/stdout
    # Debug		 		           # Write out debug messages (optional)

     MaxGap              1.5      # Maximum gap, in sample periods, allowed
                                  # between trace data points.
                                  # When exceeded, channel is restarted.

    # Specify logo(s) of the messages to grab from the InRing.
    # Up to 10 GetWavesFrom commands may be used.
    # Must specify installation ID, module ID and message type.
    # Installation and module may be wildcarded.
    # The only valid messages types are TYPE_TRACEBUF and TYPE_TRACEBUF2
    # Output message type will be the same as the input message type.
    #--------------------------------------------------------------------------
     GetWavesFrom    INST_WILDCARD MOD_WILDCARD TYPE_TRACEBUF2

    # List the 2 input SCNL codes of trace messages to compute the drift,
    # the output SCNL codes and the conversion factor.
    # If old GetSCN command is used, location code is set to "--".
    # Wildcard characters are not allowed here.
    #--------------------------------------------------------------------------
    #          Input-SCNL1      Input-SCNL2      Output-SCNL    ConversionFactor
     GetSCNL   5405 HdE NP GN   5405 HdE NP FN   5405 HrE NP GN 1.16

Module Index | Ewdrift Overview