#
Ewshear Configuration File

(last revised 31 October, 2011)

    #
    #         ewshear Configuration File
    #
     MyModuleId     MOD_EWSHEAR     # module id for this program
     InRing         TEST_RING           # transport ring to use for input
     OutRing        HYPO_RING           # transport ring to use for output
     HeartBeatInt   30                  # EW internal heartbeat interval (sec)

     LogFile        1                   # If 0, don't write logfile
     									# if 1, do (DEFAULT)
                                        # if 2, write to module log but not to
                                        # stderr/stdout
     MaxMsgSize     4096          # maximum size (bytes) for input/output msgs

    #
    # Floor definitions -- exactly one of each kind
    #   Each specifies the SCNL for that Floor's sensor
    #
     GroundFloor 5405 HNE NP ES
     TopFloor    5405 HNE NP GS

    #
    # Vertical distance between floors
    #
     Height 100

    #
    # Length of sampling window (seconds)
    #
     WindowSize 5

    #
    # Optional override of threshold for alarm
    #
    # PctShearThreshold 25	# % change in velocity to trigger alarm; default is 20

    #
    # Epsilon used in computing cross-correlation
    # Default is 0
    # Epsilon

    # Taper source data: Type Fraction
    #		Type is either BARTLETT, HANNING, PARZAN, or BMHARRIS
    #		Fraction is how much of each end of data is tapered
     Taper	HANNING 0.1

Module Index | Ewshear Overview