#
Ewaccel Configuration File

(last revised 8 June, 2011)

    #
    #         ewaccel Configuration File
    #
     MyModuleId     MOD_EWACCEL     # module id for this program
     InRing         TEST_RING           # transport ring to use for input
     OutRing        HYPO_RING           # transport ring to use for output
     HeartBeatInt   30                  # EW internal heartbeat interval (sec)
     LogFile        1                   # If 0, don't write logfile; if 1, do
                                        # if 2, write to module log but not to
                                        # stderr/stdout
     MaxMsgSize     4096          # maximum size (bytes) for input/output msgs

     DefaultConversion	0.0004673	# Optional default floor conversion value;
     								# MUST be provided BEFORE any Floor or
     								# GroundFloor command that is to use it

    #
    # Floor definitions
    #   Each specifies the mass, SCNL & conversion factor for that Floor
    #
    #   There must be exactly 1 ground floor
     GroundFloor 100 5405 HNE NP GS

    #   There can be an arbitrary number of non-ground floors, but each must have
    #   a distinct identifier (first arg to Floor command)
     Floor XE_floor 100 5405 HNN NP XE

     BaseShearThreshold 70	# force threshold to trigger alarm

     AvgWindow   2                # Number of seconds of data to use to compute

     HighPassFreq        0.075    # Cutoff frequency for high pass filter
     HighPassOrder       4        # Order for high pass filter

    # DebugForces		# Optional command to write force computations to OutRing

     AlarmDelay	3		# Required number of seconds to suspend issuing alarm messages
     					# after an alarm message has been issued

Module Index | Ewaccel Overview