# SrPar2Ew Configuration File Commands

(last revised 05 December, 2007)
Page Index:
1. Functional command listing
2. Alphabetic command listing & description
3. Sample Configuration File

On startup, SrPar2Ew reads the configuration file named on the command line. Commands in this file set all the parameters used for configuring the Earthworm SrPar2Ew module. In the control file, lines may begin with a valid SrPar2Ew command (listed below) or with one of 2 special characters:

>     #  marks the line as a comment (example: # This is a comment).

>     @  allows control files to be nested; one control file can be
>        accessed from another with the command "@" followed by
>        a string representing the path name of the next control file
>        (example: @model.d).

Command names must be typed in the control file exactly as shown in this document (upper/lower case matters!). Blank lines are also permitted in the control file.

## 1. FUNCTIONAL COMMAND LISTING

Below are the commands recognized by SrPar2Ew, grouped by the function they influence. Some of the commands are required, as noted. They may be specified in any order in the control file.

       Earthworm system setup:
                    ModuleId                required
                    RingName                required
                    LogFile                 required
                    HeartbeatInterval       required
                    OutputMsgType           optional
                    Debug                   optional

       PARxCH data acquisition parameters:
                    AtodDriverName          required
                    AtodModelName           required
                    PortMode                required
                    SamplingRate            required

       PARGPS timing module parameters:
                    GpsEnable               required
                    GpsDriverName           required
                    GpsSerialPort           required
                    GpsModelName            optional

       Summary logging parameters:
                    SummaryInterval         optional
                    GpsReportInterval       optional
                    GpsBadLimit             optional

       Channel SCNL parameters:
                    EwChannelScnl           optional
                    EwChannel               deprecated (use EwChannelScnl instead)

       2nd board PARxCH data acquisition parameters:
                    AtodDriverNameN         optional
                    AtodModelNameN          optional
                    PortModeN               optional

## 2. ALPHABETIC COMMAND LISTING & DESCRIPTION

In the following section, all configuration file commands are listed in alphabetical order. Listed along with the command (bold-type) are its arguments (in red), the name of the subroutine that processes the command, and the function within the module that the command influences. A detailed description of the command and is also given. Default values and example commands are listed after each command description.

    command arg1                                       function

    AtodDriverName driver_name                      PARxCH Configuration

> Sets the name of the PARxCH device driver to driver_name. This name is case sensitive and must match the name used when installing the driver.

>     Default:  None
>     Example:  AtodDriverName SrParXch0

    AtodDriverNameN driver_name                      PARxCH 2 Board Configuration

> Sets the name of the second PARxCH device driver to driver_name. This name is case sensitive and must match the name used when installing the driver. This keyword is only used when running with two PAR8CH + one PARGPS.

>     Default:  None
>     Example:  AtodDriverNameN SrParXch1

    AtodModelName xch_model_name                    PARxCH Configuration

> Indicates which member of the PARxCH family of 24 bit data acquisition devices is being used. xch_model_name can be PAR1CH, PAR4CH, or PAR8CH. This name is case sensitive and must match the model you are actually using.

>     Default:  None
>     Example:  AtodModelName PAR8CH

    AtodModelNameN xch_model_name                    PARxCH 2 Board Configuration

> Indicates which member of the PARxCH family of 24 bit data acquisition devices is being used as the second A/D. Both xch_model_name and the argument for AtodModelName must be PAR8CH to work correctly. This name is case sensitive and must match the model you are actually using. This keyword is only used when running with two PAR8CH + one PARGPS.

>     Default:  None
>     Example:  AtodModelNameN PAR8CH

    Debug n                                         Earthworm setup

> Sets the log output level for SrPar2Ew. Errors and warnings are always logged. Level 0 adds startup info. Level 1 adds general summaries every SummaryInterval seconds and GPS lock status summaries every GpsReportInterval seconds. Level 2 adds some additional details. Level 3 adds time and satellite info for every 1 second buffer of data. Level 4 adds NMEA messages for every buffer. Level 5, primarily for code debugging, adds function calls and program variable values.

>     Default:  0
>     Example:  Debug 1

    EwChannel n sta comp net pin                    Channel Configuration

> This command is similar to EwChannelScnl except there is no location value. Please use EwChannelScnl instead.

>     Default:  The channels are named CH## with component xxx and net SR
>               the pin number is set equal to the PARxCH channel number.
>     Example:  EwChannel 0 CH00 xxx SR 0

    EwChannelScnl n sta comp net loc pin            Channel Configuration

> There should be one EwChannelScnl command for each PARxCH channel, including special channels like the digital and GPS mark channels. This information is used to provide the full station, component, network and location names (SCNL) plus pin number as headers for the earthworm trace buffer messages. n indicates the PARxCH channel number while sta comp net loc pin give the earthworm SCNL and pin values.

>     Default:  The channels are named CH## with component xxx, net SR and
>               location -- (indicating blank location).  The pin number is
>               set equal to the PARxCH channel number.
>     Example:  EwChannelScnl 0 CH00 xxx SR -- 0

    GpsBadLimit nbad                                Summary Logging

> The GPS lock status is determined once a second (ie for every buffer of data acquired). It is defined as good if 3 or more satellites are in view, and as bad otherwise. Since there are typically many seconds in one GpsReportInterval, we need a criteria to determine if the GPS lock status summarized over the interval is good or bad. GpsBadLimit provides this criteria. If the GPS lock status was bad for more than nbad seconds during the current GpsReportInterval, the summary status is defined as bad. An error message is written to the Earthworm ring every time the summary GPS lock status changes.

>     Default:  1
>     Example:  GpsBadLimit 60

    GpsDriverName driver_name                       PARGPS Configuration

> Sets the name of the PARGPS device driver to driver_name. This name is case sensitive and must match the name used when installing the driver.

>     Default:  None
>     Example:  GpsDriverName SrParGps0

    GpsEnable on_off                                PARGPS Configuration

> This on_off switch is a case sensitive character string and must be either ON or OFF. It controls whether or not the PARGPS is used to provide precise time stamping of the data. If the PARGPS is not used, the waveform tracebuf times are determined by multiplying the sample rate by the number of samples.

>     Default:  None
>     Example:  GpsEnable ON

    GpsModelName gps_model_name                     PARGPS Configuration

> Indicates what equipment is being used to determine GPS time. Currently, gps_model_name must be GARMIN, TRIMBLE, ONCORE, or PCTIME. TRIMBLE is the default and refers to the Symmetric Research Rev C GPS timing unit that includes a Trimble Ace III receiver. GARMIN refers to the Symmetric Research Rev D GPS timing unit that works with the Garmin GPS 18 LVC. ONCORE refers to a Motorola Oncore GT+ unit (this model has been discontinued by Motorola). PCTIME means time stamping of the data is done using the PC system time and assumes this time is accurate because it has been set using NTP (Network Time Protocol) or some other GPS receiver. Other values may be allowed in the future.

>     Default:  TRIMBLE
>     Example:  GpsModelName GARMIN

    GpsReportInterval nsec                          Summary Logging

> A summary of the GPS lock status is written to the log file every nsec seconds if the log file is turned on (LogFile 1), a medium log output level is selected (Debug >= 1), and you are using GPS (GpsEnable ON). Set nsec to 0 if no GPS lock status lines are desired.

>     Default:  0
>     Example:  GpsReportInterval 1200

    GpsSerialPort n                                 PARGPS Configuration

> This integer selects which COM port is used to transfer the GPS serial NMEA strings that contain time and location to the PC. n must be 1 or 2 for serial port COM1 or COM2 respectively.

>     Default:  None
>     Example:  GpsSerialPort 1

    HeartbeatInterval nsec                          Earthworm Setup

> Defines the number of seconds, nsec, between TYPE_HEARTBEAT messages issued by SrPar2Ew.

>     Default:  none
>     Example:  HeartbeatInterval 60

    LogFile n                                       Earthworm Setup

> Sets the on-off switch for writing a log file to disk. If n is 0, no log file will be written. If n is non-zero, SrPar2Ew will write daily log file(s) called nnnnn_yyyymmdd.log where nnnnn is the name of the configuration file (with the suffix '.d' removed) and yyyymmdd is the current UTC date (ex: 20040123) on the system clock. The file(s) will be written in the EW_LOG directory (environment variable).

>     Default:  none
>     Example:  LogFile 1

    ModuleId mod_id                                 Earthworm setup

> Sets the module id for labeling all outgoing trigger, heartbeat, and error messages. mod_id is a character string (valid strings are listed in earthworm.d) that relates to a unique single-byte number. In general, a different module ID is needed for each instance of SrPar2Ew.

>     Default:  none
>     Example:  MyModuleId MOD_SRPAR2EW

    OutputMsgType trace_format                      Earthworm setup

> Tells SrPar2Ew whether to send waveform messages in the the old or new style tracebuf format. trace_format is a case sensitive character string and must be either TYPE_TRACEBUF or TYPE_TRACEBUF2. For Earthworm v7.0 and later, TYPE_TRACEBUF2 is the default.

>     Default:  TYPE_TRACEBUF2 (for v7.0 and greater, TYPE_TRACEBUF otherwise)
>     Example:  OutputMsgType TYPE_TRACEBUF2

    PortMode port_mode                              PARxCH Configuration

> Indicates which protocol is used to communicate over the PC parallel port. port_mode can be BPP, EPP, ECP/EPP, or ECP/BPP. This name is case sensitive and must match the mode your PC is actually using. Typically this setting is controlled in the BIOS CMOS setup area. Use the diagnostic program diag.exe that comes with the PARxCH to see which modes are enabled.

>     Default:  None
>     Example:  PortMode ECP/BPP

    PortModeN port_mode                              PARxCH 2 Board Configuration

> Indicates which protocol is used to communicate over the second PC parallel port. port_mode can be BPP, EPP, ECP/EPP, or ECP/BPP. This name is case sensitive and must match the mode your PC is actually using. Typically this setting is controlled in the BIOS CMOS setup area. Use the diagnostic program diag.exe that comes with the PARxCH to see which modes are enabled. This keyword is only used when running with two PAR8CH + one PARGPS.

>     Default:  None
>     Example:  PortModeN ECP/BPP

    RingName ring                                   Earthworm setup

> Tells SrPar2Ew which shared memory region to use for output. ring is a character string (valid strings are listed in earthworm.d) that relates to a unique number for the key to the shared memory region.

>     Default:  none
>     Example:  RingName WAVE_RING

    SamplingRate sps                                PARxCH Configuration

> Requests how many samples per second to acquire. The actual sampling rate may be a little different than the sps requested since only certain rates are achievable with the PARxCH hardware. Currently, the maximum allowed sps is 1000.

>     Default:  None
>     Example:  SamplingRate 100.0

    SummaryInterval nsec                            Summary Logging

> A summary of the analog, GPS PPS, and GPS serial info read is written to the log file every nsec seconds if the log file is turned on (LogFile 1) and a medium log output level is selected (Debug >= 1). The GPS information will be included only if you are using GPS (GpsEnable ON). Set nsec to 0 if no summary lines are desired.

>     Default:  0
>     Example:  SummaryInterval 1200

##
3. Sample Configuration File

    # FILE: srpar2ew.d                  Copyright (c), Symmetric Research, 2004-2010
    #
    # This is the SrPar2Ew parameter file for acquiring data with a
    # Symmetric Research PARxCH 24 bit A/D board and putting that
    # data onto an earthworm ring.
    #
    # The standard earthworm import_generic/export (or export_scnl) functions
    # can be used to transfer PARxCH tracebuf data from a local WAVE_RING to
    # a WAVE_RING on another machine.  If you have data from two different
    # PARxCH boards arriving at the same ring, you must ensure that each is
    # using a different ModuleId.  Otherwise, the two sets of data will
    # appear to be scrambled together which leads to lots of message sequence
    # number errors.
    #
    # If you wish to use MOD_SRPAR2EW for a ModuleId instead of
    # MOD_ADSEND_C, you must first define it in your earthworm.d file.
    #

    Debug               2               # control amount of info sent to log file 0-8
                                        # warnings and errors always given
                                        # 0 adds startup info
                                        # 1 adds status summaries every GpsReportInterval
                                        # 2 adds config + more detail (default)
                                        # 3 adds trace data message info every second
                                        # 4 adds counter values, NMEA strings every second
                                        # Remaining levels 5-8 mostly for code debugging

    #
    # Basic Earthworm parameters:
    #

    MyModuleId         MOD_ADSEND_C     # module id for this instance of SrPar2Ew
    RingName           WAVE_RING        # shared memory ring for outputting acquired data
    LogFile            1                # 0 to turn off disk log file; 1 to turn it on
    HeartBeatInterval  60               # seconds between heartbeats, only checked
                                        # after each second of data is acquired
    #
    # Optional Earthworm parameters:
    #

    OutputMsgType   TYPE_TRACEBUF2      # Older style waveforms were identified by
                                        # Station/Channel/Network (SCN), the newer
                                        # style also includes Location.  For Earthworm
                                        # v7.0 and greater use, TYPE_TRACEBUF2.  If
                                        # you need the older style, use TYPE_TRACEBUF.

    #
    # Basic PARxCH parameters:
    #

    AtodDriverName     SrParXch0        # name of PARxCH kernel mode device driver installed
    AtodModelName      PAR4CH           # which PARxCH is being used: PAR1CH, PAR4CH, PAR8CH
    PortMode           ECP/BPP          # protocol used for PC parallel port communications

    SamplingRate       100.0            # requested sampling rate - the actual rate may be
                                        # slightly different from this due to hardware
                                        # considerations

    #
    # Basic PARGPS parameters:
    #

    GpsEnable          ON               # ON if using PARGPS, OFF otherwise
    GpsDriverName      SrParGps0        # name of PARGPS kernel mode device driver installed
    GpsModelName       PARGPS           # usually PARGPS, may be PCTIME for NTP time
    GpsSerialPort      1                # COM port being used for serial NMEA messages

    #
    # Optional logging parameters:
    #
    SummaryInterval   1200              # seconds in log file between summary info
                                        # use 0 for no reporting
    GpsReportInterval 3600              # seconds in log file between GPS lock lines
                                        # use 0 for no reporting
    GpsBadLimit        300              # number of bad locks allowed per interval
                                        # before error message is sent

    #
    # Channel info: SCNL AND PIN VALUES FOR EACH A/D CHANNEL
    #
    # EwChannelScnl lines relate the PARxCH channel numbers to the SCNL and pin
    # numbers used to identify channels in an earthworm system.  The pin
    # numbers are optional.  If a pin number is not specified for a channel,
    # the pin number is set to the A/D channel number.
    #
    # Three different versions of this section are given below showing how
    # the setup would look when using the PAR1CH, PAR4CH, or PAR8CH.  Only
    # the version corresponding to the PARxCH you are actually using should
    # be commented in, the other two should be commented out.
    #
    # The older keyword EwChannel is the same, except it has no location value.
    # If OutputMsgType = TYPE_TRACEBUF2 and EwChannel is used, the location field
    # defaults to "--" which means a blank location.
    #

    #
    # Sample EwChannelScnl section for the PAR1CH
    #

    #              A/D
    #            Channel   Sta   Comp  Net  Loc  Pin
    #            -------   ---   ----  ---  ---  ---
    #EwChannelScnl   0      CH00  xxx   SR   --    0
    #EwChannelScnl   1      MARK  xxx   SR   --    1   # Include this when using PARGPS

    #
    # Sample EwChannelScnl section for the PAR4CH
    #

    #              A/D
    #            Channel   Sta   Comp  Net  Loc  Pin
    #            -------   ---   ----  ---  ---  ---
    #EwChannelScnl   0      CH00  xxx   SR   --    0
    #EwChannelScnl   1      CH01  xxx   SR   --    1
    #EwChannelScnl   2      CH02  xxx   SR   --    2
    #EwChannelScnl   3      CH03  xxx   SR   --    3
    #EwChannelScnl   4      MARK  xxx   SR   --    4   # Include this when using PARGPS

    #
    # Sample EwChannelScnl section for the PAR8CH
    #

    #              A/D
    #            Channel   Sta   Comp  Net  Loc  Pin
    #            -------   ---   ----  ---  ---  ---
    #EwChannelScnl   0      CH00  xxx   SR   --    0
    #EwChannelScnl   1      CH01  xxx   SR   --    1
    #EwChannelScnl   2      CH02  xxx   SR   --    2
    #EwChannelScnl   3      CH03  xxx   SR   --    3
    #EwChannelScnl   4      CH04  xxx   SR   --    4
    #EwChannelScnl   5      CH05  xxx   SR   --    5
    #EwChannelScnl   6      CH06  xxx   SR   --    6
    #EwChannelScnl   7      CH07  xxx   SR   --    7
    #EwChannelScnl   8      DGTL  xxx   SR   --    8
    #EwChannelScnl   9      MARK  xxx   SR   --    9   # Include this when using PARGPS
    #EwChannelScnl  10      CNTR  xxx   SR   --   10   # Include this when using PARGPS

    #
    # Actual EwChannelScnl section being used ...
    # replace with appropriate values for your installation
    #

    #              A/D
    #            Channel   Sta   Comp  Net  Loc  Pin
    #            -------   ---   ----  ---  ---  ---
    EwChannelScnl   0      CH00  xxx   SR   --    0
    EwChannelScnl   1      CH01  xxx   SR   --    1
    EwChannelScnl   2      CH02  xxx   SR   --    2
    EwChannelScnl   3      CH03  xxx   SR   --    3
    EwChannelScnl   4      MARK  xxx   SR   --    4   # Include this when using PARGPS

Module Index | SrPar2Ew Overview