# Earthworm Modules:
RayLoc_ew Configuration File

(last revised 13 July, 2004)
On startup, rayloc_ew reads the configuration file named on the command line. In the control file, lines may begin with a valid rayloc_ew commands (listed below).
# marks the line as a comment (example: # This is a comment).
Command names must be typed in the control file exactly as shown in this document (upper/lower case matters!). Blank lines are also permitted in the control file.

## 1. FUNCTIONAL COMMAND LISTING

Below are the commands recognized by liss2ew, grouped by the function they influence. Most of the commands are required; they may be specified in any order in the control file.

Earthworm system setup

                    MyModId          required
                    HeartbeatInt     required
                    InRing           required
                    OutRing          required
                    Debug            optional

Rayloc processing parameters:

                    StaFile        required
                    WorkDir        required

                    hold_params           optional; default if absent = 0
                    fix_depth             optional; default if absent = 1
                    use_PKP               optional; default if absent = 1
                    use_depth_ph          optional; default if absent = 1
                    use_S_ph              optional; default if absent = 1
                    pick_weight_interval  optional; default if absent = 0
                    Rmin                  optional; default if absent = 0
                    Rmax                  optional; default if absent = 0

                    D1                    optional; default if absent = 0
                    Dmin1                 optional; default if absent = 0
                    Dmax1                 optional; default if absent = 180

                    D2                    optional; default if absent = 0
                    Dmin2                 optional; default if absent = 0
                    Dmax2                 optional; default if absent = 180

                    D3                    optional; default if absent = 0
                    Dmin3                 optional; default if absent = 0
                    Dmax3                 optional; default if absent = 180

                    D4                    optional; default if absent = 0
                    Dmin4                 optional; default if absent = 0
                    Dmax4                 optional; default if absent = 180

                    D5                    optional; default if absent = 0
                    Dmin5                 optional; default if absent = 0
                    Dmax5                 optional; default if absent = 180

## 2. ALPHABETIC COMMAND LISTING & DESCRIPTION

In the following section, all configuration file commands are listed in alphabetical order. Listed along with the command (bold-type) are its arguments (in red), the name of the subroutine that processes the command, and the function within the module that the command influences. A detailed description of the command and is also given. Default values and example commands are listed after each command description.

    command arg1                                 processed by             in function

    D1,D2,D3,D4,D5   0 or 1    rayloc_ew_GetConfig              processing parameters

> Pick weight distance interval flag(s) (there are five parameters 1=5) (TRUE = 1/FALSE = 0) (def = 0)

>     Default:  0
>     Example:  D1 0
>               D2 1
>               D4 1

    Debug                                           rayloc_ew_GetConfig              Earthworm setup

> Turns on debug logging for rayloc_ew.

>     Default:  no debug logging
>     Example:  Debug

    Dmin1, Dmin2, Dmin3, Dmin4 Dmin5 degrees                        rayloc_ew_GetConfig              processing parameters

> Lower bound of distance interval(s) in which weights are zero (default 0). Note that in order to use this parameter, a corresponding Dx should be turned ON.

>     Default:  0
>     Example:  Dmin1 0
>               Dmin2 10
>               Dmin5 20

    Dmax1, Dmax2, Dmax3, Dmax4, Dmax5    degrees                         rayloc_ew_GetConfig              processing parameters

> Upper bound of distance interval(s) in which weights are zero (default 180). Note that in order to use this parameter, a corresponding Dx should be turned ON.

>     Default:  0
>     Example:  Dmax1 180
>               Dmin2 170
>               Dmin5 160

    fix_depth       0 or 1                         rayloc_ew_GetConfig              processing parameters

> Use fixed depth in inversion: TRUE (1) or FALSE(0).

>     Default:  1
>     Example:  fix_depth 1

    HeartBeatInt nsec                         rayloc_ew_GetConfig             Earthworm Setup

> Defines the number of seconds, nsec between TYPE_HEARTBEAT messages issued by rayloc_ew.

>     Default:  none
>     Example:  HeartBeatInterval 30

    hold_params   0 or 1                         rayloc_ew_GetConfig             processing parameters

> Hold latitude, longitude, depth, and origin time flag (default = FALSE (0).

>     Default:  0
>     Example:  hold_params 1

    InRing ring                            rayloc_ew_GetConfig              Earthworm setup

> Tells rayloc_ew which shared memory region to use for input. ring is a character string (valid strings are listed in earthworm.d) that relates (in earthworm.d) to a unique number for the key to the shared memory region.

>     Default:  none
>     Example:  InRing HYPO_RING

    MyModId mod_id                        rayloc_ew_GetConfig              Earthworm setup

> Sets the module id for labeling all outgoing trigger, heartbeat, and error messages. mod_id is a character string (valid strings are listed in earthworm.d) that relates to a unique single-byte number.

>     Default:  none
>     Example:  MyModuleId MOD_RAYLOC_EW

    OutRing ring                             rayloc_ew_GetConfig              Earthworm setup

> Tells rayloc_ew which shared memory region to use for output. ring is a character string (valid strings are listed in earthworm.d) that relates (in earthworm.d) to a unique number for the key to the shared memory region.

>     Default:  none
>     Example:  OutRing PICK_RING

    pick_weight_interval 0 or 1                  rayloc_ew_GetConfig              processing parameters

> Pick weight residual interval flag (TRUE/FALSE) (default = FALSE)

>     Default:  0
>     Example:  pick_weight_interval   1

    Rmin seconds                  rayloc_ew_GetConfig              processing parameters

Lower bound of residual interval in which weights can be non-zero (default = 0). To activate this parameter pick_weight_interval must be 1.

>     Default:  0
>     Example:  Rmin 0.1

    Rmax seconds                  rayloc_ew_GetConfig              processing parameters

> Upper bound of residual interval in which weights can be non-zero (default = 0). To activate this parameter pick_weight_interval must be 1.

>     Default:  0
>     Example:  Rmax 1

    StaFile filename                  rayloc_ew_GetConfig              processing parameters

> File with stations information in GLASS format. Here is an example of few lines

>     AAE    9.0291N  38.7655E 2442 IU Addis Ababa, Ethiopia
>     AAK   42.6390N  74.4940E 1645 II Ala-Archa, Kyrgyzstan
>     AAM   42.2997N  83.6561W  249 US Ann Arbor, Michigan, USA
>     ABKT  37.9303N  58.1188E  678 II Alibek (Geyokcha), Turkmenistan
>     ABL   34.8508N 119.2208W 1981 NC Mount Abel, California, USA

> The sample file is provided with the rayloc_ew distribution. This file used to match the station names from TYPE_LOC_GLOBAL
> with their 3D coordinates (which is not a part of the TYPE_LOC_GLOBAL message).

>     Default:  none
>     Example:  StaFile        "/home/ilya/rayloc_work/glass_station_list.txt"

    use_PKP 0 or 1                  rayloc_ew_GetConfig              processing parameters

> Use or not PKP phases.

>     Default:  1
>     Example:  use_PKP 0

    use_depth_ph 0 or 1                 rayloc_ew_GetConfig              processing parameters

> Use or not depth phases.

>     Default:  1
>     Example:  use_depth_ph 0

    use_S_ph 0 or 1                  rayloc_ew_GetConfig             processing parameters

Use or not S phases.

    Default:  1
    Example:  use_S_ph 0

    WorkDir dirname                  rayloc_ew_GetConfig             processing parameters

> This is the location of the work directory for rayloc_ew. rayloc_ew stores temp files in there.
> Three model files should be placed in this directory before processing:
> 1) tau.table
> 2) ak135.hed
> 3) ak135.tbl

> Those files are prebuilt and shipped with rayloc_ew distribution.

>     Default:  none
>     Example:  WorkDir        "/export/home/isti/model"

##
3. Sample Configuration File

    #
    #                     rayloc_ew Configuration File
    #
    MyModId        MOD_RAYLOC_EW   # This instance of rayloc_ew
    StaFile        "/home/ilya/rayloc_work/glass_station_list.txt"   # File containing station information
    WorkDir        "/home/ilya/rayloc_work"         # Directory where model and tmp files are stored
    InRing           HYPO_RING     # Transport ring to find TYPE_LOC_GLOBAL messages,
    OutRing          PICK_RING     # Transport ring to write TYPE_RAYLOC messages
    HeartbeatInt            30     # Heartbeat interval, in seconds,
    Debug                    1     # If 1, print debugging message
    #
    #
    # Parameters/flags used to control processing of rayloc
    # Default values are provided in comments and used if any
    # of the parameters in to configuration is undefined
    #
    hold_params           0    # Hold latitude, longitude, depth, and origin time flag (def = 0)
    fix_depth             1    # Fix depth (def = 1)
    use_PKP               1    # Use PKP phases (def = 1)
    use_depth_ph          1    # Use depth phases (def 1)
    use_S_ph              1    # Use S phases (def = 1)
    pick_weight_interval  0    # Pick weight residual interval flag (T/F) (def = 1)
    Rmin                  0    # Lower bound of residual interval in which weights can be non-zero (def = 0)
    Rmax                  0    # Upper bound of residual interval in which weights can be non-zero (def = 0)
    #
    D1                    0    # Pick weight distance interval flag(s) (T/F) (def = 0)
    Dmin1                  0    # Lower bound of distance interval(s) in which weights are zero (def = 0)
    Dmax1                180    # Upper bound of distance interval(s) in which weights are zero (def = 180)
    #
    D2                    0   # Pick weight distance interval flag(s) (T/F) (def = 0)
    Dmin2                 0   # Lower bound of distance interval(s) in which weights are zero (def = 0)
    Dmax2               180   # Upper bound of distance interval(s) in which weights are zero (def = 180)
    #
    D3                    0   # Pick weight distance interval flag(s) (T/F) (def = 0)
    Dmin3                 0   # Lower bound of distance interval(s) in which weights are zero (def = 0)
    Dmax3               180   # Upper bound of distance interval(s) in which weights are zero (def = 180)
    #
    D4                    0   # Pick weight distance interval flag(s) (T/F) (def = 0)
    Dmin4                 0   # Lower bound of distance interval(s) in which weights are zero (def = 0)
    Dmax4               180   # Upper bound of distance interval(s) in which weights are zero (def = 180)
    #
    D5                    0   # Pick weight distance interval flag(s) (T/F) (def = 0)
    Dmin5                 0   # Lower bound of distance interval(s) in which weights are zero (def = 0)
    Dmax5               180   # Upper bound of distance interval(s) in which weights are zero (def = 180)

Module Index | rayLoc_ew Overview | | TYPE_LOC_GLOBAL | TYPE_RAYLOC

The URL of this page is [http://www.isti.com/~ilya/rayloc_ew_cmd.html]
Contact: i.dricker@isti.com