Search:
wiki:v5.0
Last modified 20 months ago Last modified on 01/17/12 12:54:25

    Earthworm Release Notes V5.0

    (June 12, 2000)
    Earthworm V5.0 Release
    **********************
    6/12/00

    V5.0 Is Released
    ****************
    It can be retrieved from the Earthworm ftp site
    ftp://ghtftp.cr.usgs.gov/pub/OUTGOING/earthworm/release_v5.0

    New Features of EW V5.0
    ***********************
    Earthworm v5.0 contains an OPTIONAL Server Package. This server consists of:
            *  a DBMS Server (Oracle v8, Standard Edition),
            *  a web server (Apache), and
            *  a map server (based on GMT).
    The initial suite of functions of this server are fairly minimal, but the idea
    is that the infrastructure is in place, and we will be in good position to
    produce additional capabilities.
                    Note that the Server Package is not required to run the
    Earthworm system. If no DBMS server is available, all Earthworm functions will
    continue to operate as before, and will be supported and enhanced as before.
    There will, however, be a growing suite of features which will be available
    only if a Server is available.

    The initial set of DBMS-based server features are:
            * The DBMS is presumed to be a network-based service. That is, the DBMS
    server may reside in the local Earthworm computer, in another computer at the
    installation, or at a remote site.
            * All event data, both parametric and waveform, known to the local
    Earthworm system can be loaded into the agreed-upon DBMS servers as it is
    computed (or received).
            * An Earthworm system can send and/or accept real-time data to/from any
    number of DBMS servers (local or distant).
            * A DBMS server can support any number of concurrent, authorized
    clients.
            * All data feeds from a local Earthworm system to any DBMS servers are
    under exclusive control of the local Earthworm configuration.
            * The DBMS server supports a web site offering rapid-response,
    interactive seismicity maps. The maps, and the associated pages, provide
    graphic access to event, trace, and station data in the DBMS.
            * Event and station data, including instrument response, can be pushed
    to a browser client in SAC format. Other formats will be incorporated.
            * Archiving of parametric and waveform data.

    For additional information about the Server Package, or for installation
    assistance, please contact me.

    OTHER NEW MODULES
    *****************

    LISS2EW
    Liss2ew is the earthworm module for receiving trace data from the Live Internet
    Seismic Server. The LISS is a protocol that provides trace data in mini-SEED
    format in near-real-time over an IP link. The liss2ew module will connect to
    one LISS, read selected streams of trace data, and write that trace data into
    the earthworm transport ring.

    EW2LISS
    Ew2liss is the Earthworm module for serving Earthworm trace data in LISS (Live
    Internet Seismic Server) format. The ew2liss module will convert selected SCNs
    (station-component-network) of trace data from an Earthworm transport ring,
    convert that data to miniSEED format, and serve the data to a single LISS
    client (such as liss2ew) over a IP network connection.

    CONTRIBUTED SOFTWARE
    **************************

    The contributed software can be found at

    ftp://ghtftp.cr.usgs.gov/pub/OUTGOING/earthworm/contributed_software

    UNIVERSITY OF UTAH:
    REFTOEW: Reftoew collects data from a UNR RefTek Data Server, a disk file or
    an  Earthworm transport ring.  The data (DT) packets are forwarded to the
    Earthworm Transport layer as TRACE_BUF format packets and optionally written to
    disk as binary SAC files.

    VOLCANO PROGRAM:
    The wonderful people at CVO have modified Carlsubtrig, Trig2disk,
    Heli_standalone, and Sgram for the greater flexibility required in the volcano
    networks.

    CARLSUBTRIG: Many new options regarding how subnets are triggered and which
    stations are saved.

    TRIG2DISK:  Functions Putaway.c SudsPutaway.c and AhPutaway.c were modified to
    use the named subnets now supplied by Carlsubtrig in naming the directories.

    HELI_STANDALONE:  Ported to NT.

    SGRAM: Ported to NT.

    In addition, an NT-based Earthworm interface has been developed by CVO, which
    replaces startstop, statmgr, and provides a GUI interface to various Earthworm
    functions.

### Download in other formats:

- Plain Text