#
Ewintegrate Configuration File

(last revised 2 March, 2010)

    #
    #                     Configuration File for ewintegrate
    #
     MyModId            MOD_DEBIAS
     InRing             WAVE_RING # Transport ring to find waveform data on,
     OutRing            INTEGRATE_RING # Transport ring to write output to,
                                  # InRing and OutRing may be the same.
     HeartBeatInterval  30        # Heartbeat interval, in seconds,
     LogFile            1         # 1 -> Keep log file, 0 -> no log file
                                  # 2 -> log to file but not to stderr/stdout
    # Debug		 		           # Write out debug messages (optional)

     MaxGap              1.5      # Maximum gap, in sample periods, allowed
                                  # between trace data points.
                                  # When exceeded, channel is restarted.

    # TestMode                     # If you want Ewintegrate to compute and log
                                  # its filter coefficients and then
                                  # exit, specify "TestMode".
     AvgWindow   5                # Number of seconds of data to use to compute
                                  # the rolling average, which gets removed from
                                  # each sample.  If missing, no debiasing will be done

     DoIntegration                # Perform integration; if missing, no integration
                                  # will be performed
     HighPassFreq        0.075    # Cutoff frequency for high pass filter
     HighPassOrder       4        # Order for high pass filter
                                  # If neither of the above are specified, no
                                  # high-pass filtering will be done.  It is an
                                  # to specify exactly one of these two

    # Specify logo(s) of the messages to grab from the InRing.
    # Up to 10 GetWavesFrom commands may be used.
    # Must specify installation ID, module ID and message type.
    # Installation and module may be wildcarded.
    # The only valid messages types are TYPE_TRACEBUF and TYPE_TRACEBUF2
    # Output message type will be the same as the input message type.
    #--------------------------------------------------------------------------
     GetWavesFrom    INST_WILDCARD MOD_WILDCARD TYPE_TRACEBUF2

    # List SCNL codes of trace messages to decimate and their output SCNL codes.
    # If old GetSCN command is used, location code is set to "--".
    # Wildcard characters are not allowed here.
    #--------------------------------------------------------------------------
    #         Input-SCNL      Output-SCNL
     GetSCNL  NP2 BHE ZZ --   DEBI HHE NP BS

Module Index | Ewintegrate Overview