Search:
wiki:v5.2
Last modified 20 months ago Last modified on 01/17/12 12:55:24

    RELEASE NOTES: EARTHWORM VERSION "V5.2"

    NEW MODULES:
    ***********

    file2ring:
    new diagnostic tool. This command-line program allows the user to
    put the contents of a file into a specified Earthworm ring as a specified
    Earthworm logo (installation, moduleid, message type). LDD 2/9/2001

    gmew:
    ground-motion analyzer. Computes PGA, PGV, PGD and spectral response
    for selected channels such as broadband and strongmotion instruments.
    Writes TYPE_STRONGMOTIONII messages, and optionally writes a ShakeMap XML
    file. PNL, 3/30/01

    reboot_mss:
    This is a command line program to remotely reboot an MSS100.
    Reboot_mss is spawned by program reboot_mss_ew.  There is no configuration
    file.  The command-line syntax is:
    reboot_mss   [-q]
    The reboot_mss program logs into the telnet port (port 23) of the
    MSS100.  Then, it issues a reboot command to the MSS100 and exits.
    If "-q" is specified, the program runs in "quiet mode", and it
    doesn't write anything to stdout.   WMK 4/23/01

    reboot_mss_ew:
    This is an Earthworm module that monitors tracebuf
    messages from any number of K2's.  If data stops being received from
    a K2 for a specified amount of time (eg 10 minutes), reboot_mss_ew
    assumes that the MSS100 is hung up, and it attempts to reboot the
    appropriate MSS100 by spawning reboot_mss as a child process.
    Rebooting seems to unhang MSS100s when they hang up.  If the ethernet
    link is down, reboot_mss_ew will periodically attempt to reboot the
    MSS100.   WMK 4/23/01

    heli_ewII:  Performs the same functions as heli_ew and heli_standalone in one program.
            1. Runs on NT and Solaris.
            2. Runs as a module: Specifying earthworm parameters in its
               configuration file will cause it to become a module. It will attach to
               the specified ring, produce heartbeats, and use earthworm logging. It can
               be restarted if it asserts 'restartMe' in its .desc file.
            3. Runs as a standalone program: If no Earthworm paramters are given in the
               .d file, it will run standalone. Errors will be written to stderr.
            4. Does not try to move files to another machine. This was removed in the name
               of security and modularity. Moving the image files to a separate server machine
               is a reasonable option, but should be done by another facility. Shared disks via
               operating system features or SendFile are two options.

    MODIFICATIONS/BUG FIXES TO EXISTING MODULES:
    *******************************************
    libsrc/solaris/dirops_ew.c
    libsrc/winnt/dirops_ew.c
    Added new function rename_ew() that allows one to rename files.  If a file
    already exists with the same name as the desired target, the old file is
    overwritten.  LDD 9/28/2000

    Added new function RecursiveCreateDir() that will create a directory along
    withall of the parent directories that are required.  Written by Carol
    Bryan. 04/05/2001

    sendmail.c
    A bug fix to libsrc/solaris/sendmail.c: it was doing a free() on a
    declared array. This seemingly fixed a problem with statmgr. Problem was
    that statmgr on Solaris would exit if the mail address didn't have enough
    periods in it. (!) Alex 3/16/1

    Mem_circ_queue
    Replaced queue_max_size.o with mem_circ_queue.o in the following
    makefiles:
      data_exchange/vdl/SCRIPTS/makefile.sol_ew
      display/sgram/makefile.sol
      seismic_processing/eqbuf/makefile.sol
      seismic_processing/eqbuf/makefile.nt
    DavidK 2001/04/12

    gaplist:
    Program now ignores the InBufl parameter.  The trace buffer length is set
    to MAX_TRACEBUF_SIZ from the file trace_buf.h.  gaplist also ignores the
    MaxScn parameter.  Any number of Scn lines are permitted.  The gap bins
    are also changed. WMK 4/19/01

    wave_serverV
    Fixed a bug in serve_trace.c: if a tank file was closed by the
    main thread while a server thread was accessing it, the next I/O error
    that the server thread saw would send it to the "abort" section of
    _writeTraceDataAscii or _writeTraceDataRaw. Here a call to fseek() would
    fail and lead to an endless loop of failed fseek calls. The fseek calls
    weren't necessary, so I removed them. PNL 10/4/2000

    Added error responses to wave_serverV routines that reply to client
    requests.  Wave_serverV now issues an error response to the client when
    an error occurs while handling the client's request.  There are two
    types of error replies, general ones that start with "ERROR ", and
    specific replies where the error is described by one of three new
    flags: FN, FB, or FC.  See comments at top of  wave_serverV.c for
    more info. DK 01/08/2001

    Added code to issue status messages when hard errors occur on tanks
    (previously a log message was issued on reads, and the program exited
    on errors from write.) Davidk 01/19/2001

    Added ability to continue to operate after failure of a single tank
    (previously wave_serverV executed on a tank write error.)  Continuance
    is controlled by a new config file param: #AbortOnSingleTankFailure.
    See README.changes in wave_serverV source directory for more info.
    Davidk 01/19/2001

    wave_viewer:
    Modified to handle new wave_serverV error response

    flags. The only noticable change to the end user should be when

    the user chooses to view a group of traces (Group tab from Menu
    Bar), and one or more of the channels in the group is unavailable.
    In previous releases, wave_viewer would just hang, now wave_viewer
    will recognize the channel as being unavailable from the
    wave_server but will continue to retrieve data for other
    channels from the server.  New version is 1.23 DK 01/08/2001

    k2ew:
    The program now calculates how long it's been since the GPS

    receiver locked to the satellites.  If greater than GPSLockAlarm

    hours, k2ew logs a warning and sends a message to statmgr.
    If the GPS synchs up later, k2ew will send another message to
    statmgr. WMK 11/7/00

    When the DontQuit parameter is set, the program now doesn't quit
    if it can't connect to the MSS100.  Instead, it retries the connection
    forever.  I also made cosmetic changes to the k2ew log file format.
    WMK 11/29/00

    gaplist:
    The program accepts a new, optional configuration parameter,

    ReportDeadChan.  If a channel is dead for more than ReportDeadChan

    minutes, gaplist will send a message to statmgr.  In the gap table,
    if there is one star in the "Dead" column, it means the channel has
    been dead less than ReportDeadChan minutes.  If there are two stars
    in the "Dead" column, it means that the channel has been dead for more
    than ReportDeadChan minutes, and that an error message has been sent
    to statmgr.  WMK 11/20/00

    eqfilter:
    Removed several unnecessary objects and system libraries

    from the link line of both makefiles. Since eqfilter doesn't talk to

    wave_servers, there is no need to link in the ws_clientII routines
    or the earthworm or system socket stuff. PNL 11/30/00
              Fixed bug that caused eqfilter to ignoring event messages
    if tport_getmsg returned GET_MISS or GET_NOTRACK.  LDD 4/26/2001

    libsrc/winnt/time_ew.c:
    timegm_ew did not work correctly unless the system
    timezone was set to GMT; this is becuase _tzset() was not called before
    the call to mktime(). It turns out that the changes that timegm_ew was
    making to the TZ environment variable were completely unnecessary. The
    result is that timegm_ew is now much simpler. PNL 11/30/00

    carlstatrig:
    changed ProcessTraceMsg() in protrace.c to log an error and

    return 0 immediately if WaveMsgMakeLocal fails.  Previously, it returned

    an error code which would cause carlstatrig to exit. Now carlstatrig will
    just skip the offending tracebuf msg and continue.  LDD 01/17/2001

    Fixed bugs in CopyToNew() and UpdateStation(). These bugs would

    occasionally cause NaN values to be inserted into a station LTA on
    startup,preventing that station from generating any triggers. PNL
    1/29/2001

    sniffring:
    Added printing of ascii messages.  LDD 01/22/2001

    Added fflush(stdout) so that a file actually gets written when one

    redirects stdout with >fileame.  LDD 02/13/2001

    libsrc/solaris/time_ew.c
    libsrc/winnt/time_ew.c:
    Fixed a roundoff bug in datestr23 and datestr23_local.

    These functions convert time as a double to a character string rounded to

    the nearest hundredth of a second. The bug caused times with fractional

    seconds >= 0.995 to be printed incorrectly (example: 30.99843 was being
    was being converted to 30.100 instead of 31.00). LDD 1/23/2001

    makefile.sol for many modules:
    Removed compilation flags -D_SPARC and -D_SOLARIS from CFLAGS= lines.
    These flags should be set in a user's earthworm environment setup file,
    ew_sol_sparc.cmd or ew_sol_intel.cmd.  The existence of these flags in the
    makefile was causing trouble for anyone who wanted to compile for an
    Intel Solaris platform. In carlstatrig, these flags caused 4-byte integer
    trace data to be misinterpreted as float data, resulting in NaN for most
    triggering variables. Makefile.sol was changed for the following modules:
     carlstatrig
     eqfilter
     import_generic
     q2ew
     sac2hypo
     sm_file2ring
     sm_reftek2ew
     template
     trig2disk
     waveman2disk
    LDD 1/31/2001

    libsrc/util/tankputaway.c:
    removed a bunch of code that made a failed attempt

    to multiplex TRACEBUF messages. Now tankputaway.c writes all packets to

    disk in the order they are received. Use "remux_tbuf", a contributed
    program from Menlo PArk, to multiplex the output of tankputaway.c to
    make a file that can be read by tankplayer. PNL, 3/27/01

    naqs2ew:
    added functionality to convert Nanometrics compressed data packets

    into Earthworm tracebuf messages (previously only worked with
    Nanometrics uncompressed data packets). Earthworm messages created from
    compressed NMX packets will be of varying length, with the maximum number
    of samples per packet configurable. Earthworm messages created from
    NMX uncompressed packets are generally 1 second long. LDD 4/3/2001

    arc2trig:
    fixed bug that made it crash on terminate: the trig file was

    being closed unconditionally, but it wasn't always opened. PNL 4/7/01

    libsrc/winnt/makefile.nt and libsrc/util/makefile.nt:
    revised to make them work like real makefiles. Dpendencies are now checked
    so that compilation proceeds only if it is really needed.  PNL 4/11/01

    localmag:
    renamed site.c and site.h to lm_site.c/lm_site.h, to avoid

    confusion with similar files in libsrc/utils.  PNL 4/11/01

    carlsubtrig:

    putaway:
    deleted two obsolete variables formerly used only by sudsputaway

    from the PA_next_ev argument list; replaced them with a new variable used
    to carry subnet names to sudsputaway CJB 3/21/01

    sudsputaway:
    Added option to use subnet names in the filename; also, limit

    eventid to 3 characters. CJB 3/21/01

    trig2disk and waveman2disk:
    major overhaul to fix bugs, improve efficiency.

    Moved the xdr* and related files (used only by NT for ahputaway) to
    libsrc/winnt/rpc. Reorganized the putaway include files so that
    format specific header information is in sachead.h, while putaway-specific
    items are in *putaway.h All the function prototypes used to access the
    format-specific putaway routines is in pa_subs.h. Created putaway.h, that
    lists the function prototypes for the main putaway routines. Reformated
    the code so most of it isn't tabbed acorss the page; revised many
    comments.
    See src/archiving/waveman2disk/Changes for more details. See also the
    changes to each of the config files, listed below. PNL 4/12/01

    hyp2000_mgr:
    Added the 200, COP, and CAR commands to the hyp2000 startup

    section.  This forces hyp2000 to use the formats produced and expected

    by other Earthworm modules. It eliminates the need for these commands
    to be listed in the user's standard hypoinverse startup file.
    LDD 4/18/01

    reboot_mss:
    The program now uses the MSS100 remote console port (7000),

    instead of the telnet port (23).  Univ of Washington can't use port 23
    at K2 sites behind firewalls.  WMK 4/26/01

    Added the -l option, which logs out the MSS100 serial port
    rather than rebooting the MSS100.  Logging out the serial port is faster
    than rebooting.  WMK 4/26/01

    reboot_mss_ew: Added new configuration file parameter (Logout).  If Logout
    is set to 1, reboot_mss_ew will log out the MSS100 serial port rather than
    rebooting the MSS100.  Logging out the serial port is faster than rebooting.
    WMK 4/26/01

    CARLSUBTRIG: Changes made to support new features:

    earthworm.h:
    new definition: MAX_SUBNET_LEN - defines the length of the name of
    subnets optionally read in carlsubtrig. The value of MAX_SUBNET_LEN is
    currently set to 10 (i.e., a subnet name of 9 characters terminated
    with a null character).

    parse_trig.h:
    The Snippet structure has been expanded to include a
    subnet[MAX_SUBNET_LEN] variable. The variable subnet[i] contains the name
    of the ith subnet defined in carlsubtrig.

    Parse_trig.c:
    Modified to look for and read the optional subnet variable.

    carlsubtrig.c:
    1) subnets:
    a) Non-numeric subnet names (currently <= 9 characters in length) read
    in carlsubtrig are now stored and passed through to later routines through
    the triglist2k message. Subnet names are optional. If the subnet name
    read from carlsubtrig.d is numeric, no subnet is passed through to later
    routines. Currently the subnets are used only in filenames written in
    sudsputaway.
    b)  If several subnets trigger simultaneously, but still less than the
    Allsubnets parameter, the subnet code of the last triggered subnet in the
    list in the input file will be used for the Subnet.  Therefore, if you
    have nested subnets (say a dome subnet and a volcano subnet), the larger
    subnet should be listed after the smaller in the input file.
    c)  If the number of subnets triggered is sufficient to meet or exceed
    the Allsubnets parameter, the Subnet field of the triglist2k message
    will default to "Regional".

    2) A "|" symbol can be used in the list of stations to differentiate those
    stations to be used in the trigger count (stations to the left of "|")
    and those stations that are not.  All stations in a subnet are recorded
    if sufficient stations to the left of the "|" are triggered.
    If no "|" symbol is present, behavior defaults to that of previous
    versions of the program.

    putaway.c:
    PA_next_ev carried two arguments that were used only by sudsputaway.
    With the new subnet variable, these two variables are now obsolete,
    and have been deleted. The subnet variable, however,  was added to the
    argument list of PA_next_ev. The prototype of PA_next_ev is now:
    int     PA_next_ev (char *EventID, TRACE_REQ *trace_req, int num_req,
    int FormatInd, char *OutDir, char *EventDate,   char *EventTime,
    char *EventSubnet, int debug);

    sudsputaway.c:
    1) Subnet names (if alphanumeric) are used in the suds filenames.
    If no subnet is named, the installation name is used in the filename.
    Thus, suds filenames are of the form: yyyymmdd_hhmmss_subnet_evid.dmx.

    2)  The EventId field of the filename is set to 3 characters.
    If the EventId is greater than 999, it is truncated to the last 3 digits.
    Leading zeroes are added to numbers less than 100.

    CHANGES TO CONFIGURATION FILES and DESCRIPTOR FILES:
    ****************************************************
    k2ew:
    The configuration file now has the capability to rename the
    station coming off the k2. This is an override mechanism and allows
    the name to be specified in the .d file for legacy station names. In
    this instance, the owner of the K2 wanted to keep the name as a number
    and the institution pulling data (CalTech) processed the data using
    a station NAME. The new parameter is StationID followed by the new
    station name. The location on the k2 where this comes from is the stnid
    parameter. This was tested only under Solaris using serial communications
    and works for both restart and non-restart modes.
    PAF 4/23/2001 p.friberg@isti.com

    Configuration files contain a new optional parameter, GPSLockAlarm.
    If the GPS hasn't locked for GPSLockAlarm hours, a warning message will
    be logged and an error will be sent to statmgr.  The k2ew descriptor file
    now contains a new error for loss of GPS synch to the satellites.  WMK
    11/7/00

    gaplist:
    Configuration file contains new optional parameter: ReportDeadChan.
    If the config file doesn't contain ReportDeadChan, 10.0 minutes is the
    default value.  WMK 11/20/00

    wave_serverV.d:
    A new command was added: AbortOnSingleTankFailure
    The default behavior is the same as before, but setting
    AbortOnSingleTankFailure to 0 will cause wave_serverV
    to continue even if there is a hard error on a tank.  DK 1/19/2001

    wave_serverV.desc:
    two new error messages were added to the descriptor file.
    Error 7 is issued when a hard i/o error occurs on a
    tank or index file (this does not include a failed open).
    Error 8 is issued when a server thread cannot write a
    tank summary to the client (unless it failed because there
    was no data in the tank).  DK 1/19/2001
    #
    err: 7  nerr: 1  tsec: 0  page: 0 mail: 99
    text: "hard i/o error on tank or index file"
    #
    err: 8  nerr: 1  tsec: 0  page: 0 mail: 99
    text: "failed to write summary for a tank"

    waveman2disk.d:
    Removed TravelTimeout and MaxTraceMsg since
    they served no useful purpose.  PNL 4/12/01

    trig2disk.d:
    Removed TravelTimeout since it served no useful purpose.
    Added optional QueueSize, QueueFile for saving trigger queue to disk
    and reloading on restart.
    Added optional DelayTime to delay processing of trigger message, allowing
    for traces to arrive at the wave_server.
    Removed pin number from the TriggerStation command, since it wasn't used.
      PNL 4/12/01

    trig2disk.desc:
    added the missing error messages and their config
    parameters.  PNL 4/12/01

    gaplist.d:
    Program now ignores the InBufl parameter.  The trace buffer length is set
    to MAX_TRACEBUF_SIZ from the file trace_buf.h.  gaplist also ignores the
    MaxScn parameter.  Any number of Scn lines are permitted. WMK 4/19/01

    carlsubtrig.d:
    A "|" symbol can be used in the list of stations to differentiate those
    stations to be used in the trigger count (stations to the left of "|") and
    those stations that are not.  All stations in a subnet are recorded if
    sufficient stations to the left of the "|" are triggered. If no "|" symbol
    is present, behavior defaults to that of previous versions of the program.

    KNOWN BUGS or DEFICIENCIES:
    **************************
    In Windows NT, the time resolution of sleep_ew() is about 16 msec (one clock
    tick).  On Solaris, the resolution is about 10 msec.  This is a problem for
    ringtocoax, since packet delays need to be set to a few milliseconds.

    Automatic restarts of adsend (using the "restartMe" line in the descriptor
    file) can cause an NT system to hang. Therefore, you should never
    use the autorestart feature with adsend, but you should bring down
    the entire Earthworm system if adsend needs to be restarted.
    LDD 5/31/2000 Comments added to adsend.desc, but leave this warning here!

    statmgr: A space is needed between "tsec:" and the value.
    If it isn't there, things fail. (Alex)

    threads functions: The KillThread function on WindowsNT and Solaris
    terminate the thread without ensuring that no mutexes are held. If a thread
    holds a mutex when it dies, no other thread can get that mutex. PNL 1/12/2000

    carlsubtrig:  The system time must be set to GMT and ew_nt.cmd must have
    TZ=GMT for carlsubtrig to work.  Comments in ew_nt.cmd done 5/25/00. Barbara

    ew2seisvole: on NT, exits with horrible crash when system is stopped.

    Wave_viewer will display fictitious 2 to 3 sample gaps when scrolling the
    display.
     This does not happen all of the time and is only visible when there are less
    than
     200 samples on the display (2 seconds of data for 100hz data.) DK 2000/06/01

    libsrc/util/putaway.c: there is no include file for the putaway routines,
      thus any errors in arguments passed to putaway routines are not checked
      by the compiler.   PNL 7/10/2000

    NUMBER OF RINGS LIMITED ON SOLARIS:
    Under Solaris 2.6 (and probably other versions as well), the maximum number
    of shared memory segments is six. This means that on an out-of-the-box machine
    you can only configure six rings. If you try to configure more than that, you
    will see a cryptic message from tport_create about too many open files.  The
    fix to this problem is to add the following lines to the /etc/system
    file, and then reboot the system.

     set shmsys:shminfo_shmmax = 4294967295
     set shmsys:shminfo_shmmin = 1
     set shmsys:shminfo_shmmni = 100
     set shmsys:shminfo_shmseg = 20
     set semsys:seminfo_semmns = 200
     set semsys:seminfo_semmni = 70

    This allows for 20 rings.

         Lucky Vidmar (7/6/2000)

    startstop_solaris: There MAY be a problem with the signal that
    startstop sends to modules during the shutdown sequence. The shutdown
    sequence is started (after typing "quit" to startstop or running "pau")
    by startstop placing a terminate message on all transport rings. Modules
    should see this message and start their own shutdown. After a configurable
    delay, startstop checks to see that all modules have exitted. Any that are
    still running are sent a signal to terminate them. Currently that signal
    is SIG_TERM. But since wave_serverV has a handler for SIG_TERM, wave_serverV
    sees that as essentially the same as a terminate message. So if wave_serverV
    is having problems completing its shutdown, SIG_TERM won't do anything. The
    result is that startstop may give up and exit, leaving wave_serverV running.
    If that happens, the operator will have to terminate wave_serverV by doing
    "kill -9 ". That may leave shared memory and semaphores
    stranded in the kernel: run the command "ipcs -a" to see. If necessary,
    the stranded shared memory and semaphores may be cleaned up with the
    ipcrc command; must be run as root; see the man page.
    This problem only exists on Solaris/Unix, not on WindowsNT.
    PNL, 10/4/2000

    libsrc/utils/kom.c: The comment above k_open() says that only one file can
    be open at a time. Yet the Kbuf array has slots for MAXBUF (currently 4) open
    files. Does this work, or is the comment to be taken at it's word?
    PNL 10/15/00

    libsrc/utils/site.c: The strings used for station, channel and network are
    required to be fixed length with trailing spaces added to short names. If
    the strings given to site_index do not have these trailing blanks, SCN names
    will not match. This is not documented anywhere.  PNL 10/15/00

    libsrc/utils/logit.c: logit_init() requires a module_id number, which it uses
    to construct the log file name. This is not helpful, since the module_id
    number is not meaningful to people. Worse, it requires that the config file be
    read and earthworm.d lookups be completed before logit calls can be made. Thus
    errors in the config file can only be reported to stderr or stdout instead of
    being saved in a file.  PNL 11/29/00

    trig2disk and waveman2disk: these two programs have a TravelTimeout option in
    their config files. This feature does not work, since the "wait time" feature
    has never been implemented in wave_serverV.  PNL 11/29/00
    FIXED PNL, 4/11/01

    TRACEBUF messages.
    The definition of `endtime' of the TRACEBUF message is not documented.
    Some programmers are taking it as the "expected start time of the next
    TRACEBUF packet (if the sample interval is uniform.)" The more accepted
    practice is that `endtime' is the time of the last sample of the current
    TRACEBUF packet; that is, one sample interval less than the expected
    start time of the next TRACEBUF messsage. Using this last definition, if a
    TRACEBUF packet has exactly one sample, then its starttime and endtime are
    the identical. Clearly this distinction needs to be documented. The file
    waveform_format (in the /home/earthworm/DOC directory) gives no specifics
    about start or end times.  PNL 1/24/01

### Download in other formats:

- Plain Text