#
Ewspectra Configuration File

(last revised 2 March, 2010)

    #
    #         ewspectra Configuration File
    #
    MyModuleId    MOD_EWSPEC # ewspectra's module id

    wsTimeout	  1000	# timeout, in seconds, for talking to waveservers

    # Waveservers to listen to: IP Port
    # Can have up to 20
    WaveServer        128.97.24.133 16022

    WSDebug       3		# Debugging level of communication w/ waveserver

    ###
    ### Specify which SCNLs to process & what operation to perform on them
    ###

    # Produce spectra from a specific SCNL
    # If writing to a ring, second SCNL is needed to be used in messages written
    PlainSpectraSCNL 5405 HNN NP GE
    #PlainSpectraSCNL 5405 HNE NP GN

    # Produce spectra from the difference between first SCNL and second
    # If writing to a ring, third SCNL is needed to be used in messages written
    #DiffSpectraSCNLs		5405 HNE NP DS 5405 HNE NP XW

    # Produce spectra from the deconvolution of the second SCNL from the first
    # If writing to a ring, third SCNL is needed to be used in messages written
    #DeconvolveSpectraSCNLs	5405 HNN NP GE 5405 HNN NP XE 5405 HNN NP S1
    #DeconvolveSpectraSCNLs	5405 HNN NP XE 5405 HNN NP GE 5405 HNN NP S2

    ###
    ### Specify timespan of data to process
    ###

    # Timespan of data to process: Start Duration
    #	Start is either YYYYMMDDHHMMSS or -S (for S seconds before now)
    #	Duration is in seconds
    #TimeSpan	-3600 29
    #TimeSpan	20110329070000 29

    TimeSpan	20110418000000 29	# 1st sample
    #TimeSpan	20110414010000 2	# 2nd sample (hour later)

    #InRing     TEST_RING	# Transport ring to find COMPUTE_SPECTRA messages on

    ###
    ### Specify options for pre-processing the timeseries data
    ### before computing the SPECTRA
    ###

    # Taper source data: Type Fraction
    #		Type is either BARTLETT, HANNING, PARZAN, or BMHARRIS
    #		Fraction is how much of each end of data is tapered
    Taper	HANNING 0.1

    # Butterworth filters: CutoffFreq Poles
    #	CutoffFreq is the cutoff frequency
    #	Poles is the number of poles used (must be an even number)
    #	LowCut = highpass filter (cut frequencies below CutoffFreq)
    #	HighCut = lowpass filter (cut frequencies above CutoffFreq)
    LowCut 		 0.1	4
    HighCut		 2.0	4

    ###
    ### Optional smoothing of SPECTRA
    ###
    Smooth	0.1				# Source data smoothing; argument is size of window in secs

    ###
    ### Specify data to include in output & where it should go
    ###

    #ReportPeaks	6	0.4	0.8		# Report the top N peaks between the two frequencies
    ReportSpectra					# Report the full computed spectra

    OutRing    HYPO_RING	# Transport ring to write SPECTRA and/or SPECTRA_PEAK messages to
    #OutFile		./ews_out.txt	# File to write spectra and/or peak info to

Module Index | Ewspectra Overview