# mseed2tbuf Configuration File

(last revised April 21, 2015)

    # The mseed2tbuf command file is very similar to the ringdup_scn command file, as
    # it's basically the same program, just compiled to read mseed in instead of tbuf2s
    #
    #  mseed2tbuf configuration file
    #
    #
     MyModuleId     MOD_MSEED2TBUF      # module id for this program
     InRing         MSEED_RING          # transport ring to use for input
     OutRing        HYPO_RING           # transport ring to use for output
     HeartBeatInt   30                  # EW internal heartbeat interval (sec)
     LogFile        1                   # If 0, don't write logfile; if 1, do
                                        # if 2, write to module log but not to
                                        # stderr/stdout
     Debug 1
    #
    # Logos of messages to export to client systems
    #              Installation       Module       Message Type
     GetMsgLogo    INST_WILDCARD   MOD_WILDCARD    TYPE_MSEED

     MaxMsgSize     4096          # maximum size (bytes) for input/output msgs
     RingSize	 100          # max# messages in outgoing circular msg buffer

    # List of station/channel/network/loc codes to duplicate.
    #--------------------------------------------------------
    # NOTE: Send_scn and Send_scn_remap commands are now obsolete, and
    # have been replaced with Send_scnl and Send_scnl_remap (which
    # include the location code field).  If the old commands are used,
    # ringdup_scn sets the location code field to * (wildcard).
    #
    # Use any combination of Send_scnl (to send data as-is) and
    #   Send_scnl_remap (to change the SCNL on the fly) commands.
    # Use * as a wildcard for any field. A wildcard in the
    #   "map to" fields of Send_scnl_remap means that field will
    #   not be renamed.
    # Use the Block_scnl command (works with both wildcards
    #   and not, but only makes sense to use with wildcards) to block
    #   any specific channels that you don't want sent.
    #   Note, the Block commands must precede any wildcard commands for
    #   the blocking to occur.
    #
    #                  send SCNL     map to SCNL
    # Block_scnl      BOZ LHZ US *                 # block this specific channel
    # Send_scnl       JMP ASZ NC 01                # send this specific channel
    # Send_scnl       JPS *   NC *                 # send all components of JPS NC
    # Send_scnl_remap JGR VHZ NC --   *   EHZ * *  # change component code only
    # Send_scnl_remap CAL *   NC *    ALM *   * *  # send all component of CAL, but
                                                   # change the site code to ALM
    Send_scnl * *  NP *

Module Index | mseed2tbuf Overview