Search:
wiki:Waveform_Message_Format
Last modified 20 months ago Last modified on 01/19/12 16:17:48

    Waveform Format

    (last revised January 7, 1999)
    /*
     * Trace_buf.h
     *
     * Header file for Earthworm packets that allow demultiplexed data
     *  from various sources to be handled efficiently. Added to
     *  Earthworm system by
     * Kent Lindquist and Roger Hansen
     * Geophysical Institute
     * University of Alaska, Fairbanks
     *
     * February, 1996
     *
     * November 1996: KGL Added net and quality fields to accommodate
     *  needs expressed by Alex Bittenbinder and the Earthworm team
     * February 1997: KGL Added pad field as used by Earthworm team
     */

    #ifndef TRACE_BUF_H
    #define TRACE_BUF_H

    #define NETWORK_NULL_STRING "-"

    typedef struct {
            int     pinno;          /* Pin number */
            int     nsamp;          /* Number of samples in packet */
            double  starttime;      /* time of first sample in epoch seconds
                                       (seconds since midnight 1/1/1970) */
            double  endtime;        /* Time of last sample in epoch seconds */
            double  samprate;       /* Sample rate; nominal */
            char    sta[7];         /* Site name */
            char    net[9];         /* Network name */
            char    chan[9];        /* Component/channel code */
            char    datatype[3];    /* Data format code */
            char    quality[2];     /* Data-quality field */
            char    pad[2];         /* padding */
    } TRACE_HEADER;

    #define MAX_TRACEBUF_SIZ 4096   /* define maximum size of trace message buffer */

    typedef union {
            char    msg[MAX_TRACEBUF_SIZ];
            TRACE_HEADER trh;
            int     i;
    } TracePacket;

    /* Byte 0 of data quality flags, as in SEED format
       ***********************************************/
    #define AMPLIFIER_SATURATED    0x01
    #define DIGITIZER_CLIPPED      0x02
    #define SPIKES_DETECTED        0x04
    #define GLITCHES_DETECTED      0x08
    #define MISSING_DATA_PRESENT   0x10
    #define TELEMETRY_SYNCH_ERROR  0x20
    #define FILTER_CHARGING        0x40
    #define TIME_TAG_QUESTIONABLE  0x80

    /* CSS datatype codes
       ******************/
    /*
            t4      SUN IEEE single precision real
            t8      SUN IEEE double precision real
            s4      SUN IEEE integer
            s2      SUN IEEE short integer
            f4      VAX/Intel IEEE single precision real
            f8      VAX/Intel IEEE double precision real
            i4      VAX/Intel IEEE integer
            i2      VAX/Intel IEEE short integer
            g2      NORESS gain-ranged
    */
    #endif

### Download in other formats:

- Plain Text