Search:
wiki:v7.1
Last modified 20 months ago Last modified on 01/17/12 12:51:56

    Earthworm Release Notes V7.1

    (April 5, 2007)
    New Modules
    Modifications/ Bug Fixes to Existing Modules
    Changes To Configuration Files And Descriptor Files
    Known Bugs
    Known Deficiencies

    Release Notes:  Earthworm Version "working"
    Cleaned out after release of v7.0 on 6/15/2006
    This release is EW V7.1 and has all of 7.0 SCNL upgrades.

    EW v7.1 released on April 5, 2007

    NEW MODULES:
    ***********

    Added data_exchange/pickwasher, a prerequisite for glass.
    Source from Hydra project, tested and documented by Mitch,
    committed and makefiles cleaned up by Stefan. Makefiles for
    Solaris and Windows only at this point.
    Stefan Lisowski 20070403

    Created a 'params' directory at the root level of Earthworm
    containing the .d and .desc files for all modules. Each
    release of earthworm will require updating these files from
    the .src tree.
    Stefan Lisowski 200704

    Added in MAC OS X flags to compile on Intel and PPC chip
    sets. This works for all my test modules except, you
    guessed it, hyp2000_mgr which doesn't compile because
    of GNU g77 or gfortran issues.
    One thing you must do for Mac OS X is to increase
    the shared memory segments by adding in a /etc/sysctl.conf
    with these settings:
    kern.sysv.shmmax=16777216
    kern.sysv.shmmin=1
    kern.sysv.shmmni=32
    kern.sysv.shmseg=16
    kern.sysv.shmall=4096
    To find out the default settings type this:
    sysctl -a | grep shm
    This work was done jointly by:
    Paul Friberg ISTI and Rae Yip (Caltech) 2007/03/28

    Added psn4putaway for PSN4 format  to libsrc/util for
    windows only, and added it to docs, trig2disk and
    waveman2disk .d files and makefile.nt's.
    Paul Friberg 2007/03/05

    Added ws2ew and psnadsend for windows for webtronics
    digitzers. These 2 modules were put in data_sources.
    Paul Friberg 2007/03/04

    tankplayer_tools/ms2tb - miniSEED to tracebuf converter
    for playing back miniSEED format time-series.
    Paul Friberg 2006/08/08

    condense_logo - Reads messages from a list of logos from one
    transport ring and writes them to another ring using its own
    installation and module id in the logo. Menlo Park
    contribution. (included/tested by Stefan 2006/11/22)

    MODIFICATIONS/BUG FIXES TO EXISTING MODULES:
    ********************************************

    q3302ew - new version based on lib330! This one
    is a vast improvement over the one based on Mountainair.
    Hal Schechner 2007/04/04

    startstop - all flavors, modified MAX_CHILD to 200 (was set
    to 100, probably to limit process usage or memory usage
    by startstop in the early days).
    Paul Friberg 2007/04/03

    localmag - 2.1.1
    INGV contributed a feature to write EVENT files in
    SHAKEMAP XML format to the SAC output directory. This optional feature
    is only usable when you also use the saveTrace option.
    Contributed by Matteo Quintiliani and Marco Oliveri of INGV.
    Integrated in with current version by Paul Friberg 2007/03/29

    diagnostic_tools/sniffwave
    Earthworm Class March 2007, added statistics flag to sniffwave
    y, n, or s options are now handled, tport function changed
    2007/03/23

    Many warnings under windows with MS 2005 compiler were
    fixed relating to time related variables using long instead
    of time_t. This had segmentation violations under some
    programs so we decided to fix all of the warnings.
    Here is the list:
    tankplayer, wave_serverV,condenselogo, ringdup, ws_clientIIx.h,
    file2ew, ringtocoax and II, config_ws, gaplist, arc2trig,
    localmag, gmew, pkfilter, statrigfilter
    Paul Friberg 2007/02/23

    archiving/trig2disk archiving/waveman2disk Solaris only
    Added Richard Luckett's support for writing miniseed format.
    This added Chad Trabant's libmseed to libsrc/util. Note
    an older version of this library is hiding in
    data_exchange/slink2ew/libslink as well. New stuff didn't
    seem to be directly backward compatible. At some point this
    shoudl be reconciled so we only have one libmseed!!
    Stefan Lisowski 2002/02/20

    diagnostic_tools/template - fixed a longstanding bug
    in template where long was used as the time type instead
    of time_t.
    Paul Friberg 2007/02/20

    lockfile_ew.c and lockfile.c added to libsrc for file locking
    for earthworm. See the lockfile.h in the include directory for
    the function declarations. Also, see the updated diagnostic_tools/template.c
    for an example of its use. The intent is to use this for
    startstop which should NEVER have more than one instance
    running per startstop_*.d file! This lockfile implementation
    works for both Windows, Linux, and Solaris (tested on each)
    Paul Friberg 2007/02/20

    data_sources/scream2ew
    scream2ew - the first call to logit_init needs to have 1 as 4th argument not the undefined config.writelog, otherwise the second call doesn't work.
    Richard Luckett
    committed to CVS by stefan 2007/02/19

    archiving/wave_serverV Linux patch
    The following patch is for wave_serverV.c to enable it to be compiled
    under linux (specifically gcc 3.3.6 doesn't seem to recognise the "#else
    if defined(...)" construct properly, at least with the default CFLAGS.
    Matthew van de Werken
    committed to CVS by stefan 2007/02/19

    seismic_processing/fir
    I believe I have discovered a bug in earthworm 7.0. It seems there
    is now a 2-byte field called version in the trace header. This is
    never set up in the fir module, so that it outputs packets to the
    transport ring with no valid information in this field. I noticed
    this when I set up a carlstatrig module which kept crashing when
    being fed with data from fir - carlstatrig checks the trace header
    for a valid version. I solved the problem by adding the lines
    outHead->version[0] = TRACE2_VERSION0;
    outHead->version[1] = TRACE2_VERSION1;
    to firfilt.c at the point where data is being copied into the
    outgoing packet.
    David Scott. 2006/9/22 (commited to CVS 2006/12/30 stefan)

    archiving/tankplayer_tools
    data_exchange/liss
    data_sources/scream2ew
    linux makefile fixes per david J Scott 20060720
    (commited to CVS 2006/12/30 stefan)

    libsrc/qlib2 - an old (10 year) version of qlib2 was in data_sources/q2ew
    We now place qlib2 in libsrc. I populated directory libsrc/qlib2
    with the qlib2 from qlib2.tar.2006.313.gz downloaded from
    http://www.ncedc.org/qug/software/ucb/ and commited the src code
    to CVS
    Ilya Dricker 2006/11/16

    evanstrig
    Fix for linux compilation.
    Laurence Withers, GSL 2006/10/23

    carlstatrig
    Michelle Kline of Utah added in STAtime as a configurable
    value (was statically set to 1 in the C code). This configuration
    is backward compatible to the old version and is an optional
    parameter. Michelle kindly updated the documentation too.
    committed to CVS 2006/10/20 Paul Friberg

    trig2disk
    Michael Lofgren of CSIRO fixed a log message bug.
    commited to CVS 2006/10/18 Paul Friberg

    gaplist:
    Changed gap- binning boundaries from 1.0 to 1.1 sec so that gaps from
    1 second timing errors will show up in a different bin from gaps caused
    by 1 missed packet (for most digital dataloggers). 2007/01/10 Lynn Dietz

    hyp2000:
    I grabbed Fred Klein's newest version of hypoinverse where he
    added the processing domain and version feature. The new command is:
    VER 'NC' '01'   / Processing domain and version
    Hypoinverse puts these two 2-character strings to the end of summary
    cards and at the top of print files. These six source files were changed:
    common.inc hycmd.for hysum.for hystl.for hyp.for hybda.for
    committed to CVS 2006/10/30 Lynn Dietz
    PS: someone needs to change hystl.fpp for Linux!!
    Incorporated Fred Klein's 11/09/2006 version of hyp2000 in which he changed
    the magnitude weight calculation from the sum of weights (float) to the
    count (int) of weighted station magnitudes.
    Committed to CVS 2007/1/4 Lynn Dietz
    Incorporated Fred Klein's 2/2007 version 1.1 of hyp2000. In this version
    Fred added the option to fix origin time (changes to common.inc, hyloc.for,
    hyp.for, hyphs.for) and did some minor tweaks to make the g77 compiler
    happy (changes to hydelt.f, hyedit.f, hyinp.for, hystl.for).
    I also removed a bunch of source files and .com files which are not
    used in either hyp2000 or hyp2000_mgr under Earthworm.
    Committed to CVS 2007/03/02 Lynn Dietz
    Incorporated Fred Klein's 3/21/2007 bug fixes. Minor logic changes in
    hyphs.for and hyloc.for related to fixing origin time or depth (which
    can now be fixed at 0.0). The program now does what the documentation
    says it will.  Committed to CVS 2007/03/23 Lynn Dietz

    hyp2000_mgr - windows issue
    The ew7.0 version of this for windows did not work properly
    due to a bad pass by value in the link to the fortran code.
    Fixed 2006/10/16 Paul Friberg

    arc2trig
    David Scott of the BGS upgrade this to be SCNL compliant. Thanks!
    commited to CVS 2006/10/13 Paul Friberg

    startstop_unix_generic.c
    Removed an fprint() from EncodeStatus() which was causing a partially
    completed EW status message to go to stderr after info from each
    child process was added to the status.  I think this was a debugging
    leftover. Lynn Dietz 2006/09/22

    gcf2ew
    Modified for TYPE_GCFSOH_PACKET output of SOH packets for SNW monitoring
    of state of health packets from guralps DM24. Same for scream2ew
    Paul Friberg, 2006/09/01
    Modified to correctly put in the TRACEBUF2 version  member values
    Paul Friberg, 2006/11/08

    q2ew
    Modified to correctly put in the TRACEBUF2 version  member values
    Ported to and tested on Linux (added makefile.ux support)
    Ilya Dricker, 2006/11/21

    scream2ew
    Modified for TYPE_GCFSOH_PACKET output of SOH packets.
    Paul Friberg, 2006/09/01
    Laurence Withers, GSL 2006/10/23 provided linux compilation fix

    grab_bag/pick_recorder - made it SCNL compliant and added
    the app to the documentation.
    Paul Friberg 2006/09/01

    tankplayer_tools/sac2tb - fixed a minor bug in the TRACE2_HEADER that
    overwrote the version element of the trace header. This bug caused
    tankplayer to barf.
    Paul Friberg 2006/08/08

    heli_ewII -- heli_ewII.h
    samp_sec now a float instead of a long to accommodate sample rates
    less than 1 Hz
    Stefan Lisowski 20060726

    scn2scnl -- to_trace_scnl.c/ scn_convert.c
    I've fixed scn2scnl so that it will truncate invalid-length SCNL strings
    and prevent strings from overrunning their bounds.  I've attached the
    files that were changed.  Both of them live in
    src\data_exchange\scn_convert.
    to_trace_scnl.c contains the fix.  The function to_trace_scnl() will now
    force the last character of each SCNL buffer to be null.  This is needed
    because strncpy will not append a null character if the source string used
    during copies is as long or longer than the number of characters to count.
    scn_convert.c has a minor fix where some local variables in s2s_com() were
    declared twice.  I removed the redundant declaration to prevent any future
    headaches.
    Mark Morrison Mon, 26 Jun 2006 15:57:19 -0600 (MDT)

    sniffwave -- sniffwave.c
    additional significant digits for sample rates < 1hz
    Stefan Lisowski 20060726

    tankplayer -- tankplayer.c
    SendLate command in tankplayer.d did not appear to be working.
    The problem is that while tankplayer will play back 3 waveform types
    (TypeADBuf, TypeTraceBuf, TypeTraceBuf2) it would only set the time
    if the type was one of the first two. Should now work for TraceBuf2 as
    well.
    John Patton (Tested, compiled and added to CVS by Stefan 20060630)

    wave_serverV -- wave_serverV.c
    The problem was that the size of the tankfile is not an integer multiple
    of the packet size and so occasionally there is a mess up at the end of
    the file (mine were 3 in this example).  The result was that the data
    requested from the server was not returned and an event file failed to
    be written.
    [Fix was to add an else to wave_serverV_config]
    Richard R Luckett, BGS (Tested, compiled and added to CVS by Stefan 20060711)
    Laurence Withers, GSL provided a fix for linux 10/23/2006

    Signals were not being handled at all under linux (which caused SIGPIPE signals
    to take down the server).  I changed some ifdefs around so that the solaris
    signal handling is compiled in under linux as well.
    Hal Schechner

    Modified behavior so that client socket-disconnects between requests are no
    longer recorded/logged as socket-errors, even when the server thinks the
    socket was not closed cleanly.  This should get rid of messages like:
    >>>> 20060210_UTC_08:51:22 Wave_serverV:ListenForMsg: Bad socket read.  iReadResult = -1
    which cause people to think an error has occurred.
    Updated server_thread.c timestamp.
    David Kragness 2006/10/09

    ws_clientIIoc / ws_clientII.h
    Upped the max menu str len (as defined by wsREPLEN) so that it is large
    enough to handle a 5000+ SCNL menu from a single wave_server.
    Downside is that it must temporarily allocate 400kb instead of 80kb when
    parsing a menu.  This seemed like a reasonable tradeoff.
    Added protection against oversized SCNL fields in wave server menus:
    increased the size of the buffers used to capture SCNL values from the
    menu, in order to reduce the chance of clobbering memory if a channel
    with SCNL longer than the spec'd tracebuf2 sizes is found in a menu.
    Fixed a bug where wsGetTraceAsciiL() was returning WS_ERR_NONE even
    though there was a warning flag (with a WS_WRN_FLAGGED) return code
    from wsParseAsciiHeaderReplyL().
    Added a work around for handling flagged wave_server returns where the
    datatype does not get properly filled in.
    DK 061906

    eqcoda:
    Modified to read per-channel parameters from more than one "StaFile".
    Final station list is sorted after all station files are input.
    Lynn Dietz 2006/09/20
    Modified to ignore channels in the "StaFile" whose pick flags are
    set to 0. Previously, those lines ended up in total count of channels.
    Lynn Dietz 2007/01/09

    pick_ew:
    Modified to be able to process multiple "StaFile" commands for setting
    per-channel picking parameters.
    Lynn Dietz 2006/09/20
    Changed name of index file to pick_ew_XXX.ndx where XXX is the moduleid
    of the current instance of pick_ew. This allows multiple instances of
    pick_ew to run on the same computer without competing for the same
    index file.
    Lynn Dietz 2006/11/16

    wave_viewer:
    Modified to accept sample rates >= 1000hz.
    David Kragness  2006/10/09
    Modified format of left-hand column so that channel naming and other
    information is more compact.
    David Kragness  2006/10/26

    sniffwave:
    Now if you give station, channel, network and location codes on command line,
    sniffwave will sniff only for TYPE_TRACEBUF2 and TYPE_TRACE2_COMP_UA
    packets. Or if you give station, channel and network, then sniffwave will
    sniff only for TYPE_TRACEBUF or TYPE_TRACE_COMP_UA. This gives you more
    control over what sniffwave looks for. However, it means you can no long sniff
    for both TYPE_TRACEBUF and TYPE_TRACEBUF2 packets at the same time with a
    single instance of sniffwave.
    Pete Lombard 2006/12/28

    scnl2scn:
    Now can perform complete mapping of SCNL names to SCN names, using
    configuration commands similar to those of scn2scnl. This is in place of the
    all-or-nothing approach of the previous scnl2scn.
    Pete Lombard 2006/12/28

    scnl2scn:
    Fixed bug in scnl2scn.c: forgot to sort the explicit list.
    Added Debug option to log the configured mapping as well as logging how it
    maps (or not) each SCNL it sees. Very verbose, so run it with Debug on only as
    long as you need it.
    Pete Lombard 2007/01/17

    naqsserTG:
    Incorporated Paul Whitmore's most recent code for processing tide gauge
    data from Nanometrics serial data streams. Paul added 5 new arguments
    to his "RequestChannel" command. See sample .d file for details.
    Lynn Dietz 2007/02/09

    wftimefilter:
    Added a sanity check on number of samples in a packet. Packets with
    nsamp <= 0 are rejected.
    Modified samplerate comparison to allow for a bit of slop before
    declaring that a samplerate has "changed." This is to allow for the
    case where a datasource is reporting the actual sample rate instead
    of nominal sample rate.
    Re-worded the logic of the if() statements which limit the logging
    of bad packets and warnings.
    Lynn Dietz 2007/02/14

    CHANGES TO CONFIGURATION FILES and DESCRIPTOR FILES:
    ****************************************************
    ****************************************************

    scnl2scn:
    Now requires commands to specify the mapping from SCNL to SCN. The commands
    are very similar to those used by scn2scnl. See the comments in scnl2scn.d
    Pete Lombard 2006/12/28

    scnl2scn:
    Added Debug option to log the configured mapping as well as logging how it
    maps (or not) each SCNL it sees. Very verbose, so run it with Debug on only as
    long as you need it.
    Pete Lombard 2007/01/17

    KNOWN BUGS:
    ***********

    liss2ew:
    liss2ew has been observed intermittantly producing malformed
    TRACE_BUF messages.  Currently the conditions for causing this problem
    are unknown.  Due to this, liss2ew should be treated as suspect.  Use at
    your own risk.  JMP 6-18-2003

    k2ew:
    k2ew uses the k2hdr.rwParms.misc.channel_bitmap parameter to decide
    which channels it will see as streams from the K2.  This is actually the
    parameter which the K2 uses to decide which channels to record in an event
    file (see K2's  command).  The K2's  is the parameter
    that shows which channels the K2 is streaming out.  This is the parameter
    that k2ew should be using to decide what data it will see.  The big problem
    is that none of the header files from Kinemetrics (nkwhdrs.h) seem to
    show this parameter anywhere. This issue is only a problem for those folks
    who want to record more channels on the K2 than they want to stream continuously.
    Terry Dye (Univ of Utah) discovered this problem when trying to stream only
    3 channels of a 12 channel K2.  LDD 4/11/2002    FIXED PNL, 6/9/03

    wave_serverV:
    it occasionally sends the following error to statmgr:
    UTC_Thu Sep 06 03:30:14 2001  WSV1/wave_serverV_nano ReadBlockData
    failed for tank [z:\nano57.tnk], with offset[999908] and record
    size[64]! errno[0] Mail sent.
    The nominal tank size is 1 megabyte, and the actual tank size is 999908.
    It looks like waveserver is trying to read off the end of the tank.
    WMK 9/6/01

    wave_serverV:
    appears not to reply to requests for a single sample of data. I noticed
    when testing wave_viewer, that if the start time and end time of a request were
    equal (in which case there should be one sample of data) then wave_serverV did
    not reply to the request (ASCII request) at all. No Data, No Flags, No Reply,
    No Nothing.  It needs to issue a reply to every request.
    DavidK 09/25/01

    wave_serverV:
    Wave server appears to be limited (on 32-bit systems) to 1GB tank sizes.
    A bug (a signed integer overflow of tmpoE at Line 1155 of
    serve_trace.c  (LocateRoughOffset()))
    prevents data retrieval from the tank under certain conditions when the
    tank size exceeds 1 GB.
    DavidK & PNL 09/27/04

    Automatic restarts of adsend (using the "restartMe" line in the descriptor
    file) can cause an NT system to hang. Therefore, you should never
    use the autorestart feature with adsend, but you should bring down
    the entire Earthworm system if adsend needs to be restarted.
    LDD 5/31/2000 Comments added to adsend.desc, but leave this warning here!

    libsrc/utils/site.c: The strings used for station, channel and network are
    required to be fixed length with trailing spaces added to short names. If
    the strings given to site_index do not have these trailing blanks, SCN names
    will not match. This is not documented anywhere.  PNL 10/15/00

    socket_ew: (libsrc/util/socket_ew_common.c libsrc/solaris/socket_ew.c
        libsrc/winnt/socket_ew.c include/socket_ew.h)
    Fixed a bug in the connect_ew function().
    When run in non-blocking mode (clients connecting to
    a server - using a timeout value), there was a bug in
    the connection code(discovered on Solaris) that caused
    the function to return a timeout-error when there was
    any kind of error during connection.
    The bug was discovered when connecting to a non-existent socket.
    When trying to connect to a non-existent wave_server on a machine,
    the underlying socket library was returning a Connection-Refused error,
    but the socket_ew library was passing back a timeout error.
    -
    The change only applies when a socket-error occurs while the function is
    waiting for the connect to happen.  The instance where you will most-likely
    see a difference, is when you try connecting to a non-existent socket.
    Previously the function would return TIMEOUT, now it will return
    connection REFUSED.
    -
    Added a new function: socketSetError_ew(),
    and defined a new socket_ew return code: CONNREFUSED_EW.
    DK 2003/02/04

    sm_ew2ora:
    There is a bug in sm_ew2ora that involves having multipe time intervals for
    components and channels.  If a strong motion message containing information
    for a channel that the DB has never seen before is loaded into the DB, and
    then later another message for the same channel with an earlier timestamp
    is loaded, the load of the second message will fail, due to problems with
    overlapping time intervals, and the call that sm_ew2ora uses to create
    those time intervals.  This problem only affects stations that were
    not previously loaded via one of the station loader programs stalist*2ora,
    and only when receiving SM data that is timestamped with a time that is
    prior to the original time for that channel.  The bug lies in the logic
    of ewdb_api_PutSMMessage(), and not in the underlying code.
    Davidk 05/25/01

    A change was made to ewdb_api_PutSMMessage() that dramatically affects
    sm_ew2ora.  Please see the note about that function.  Davidk 2001/07/26

    ewdb_api_CreateWaveform()  (ewdb_internal_CreateSnippet.c
    		    ewdb_internal_CreateWaveformDesc.c)
    Added a call to release the cursors used by the internal functions, when they
    fail.  Fixes a bug which resulted in a DB cursor leak when a call to stuff
    a snippet into the DB failed.
    DK 2003/02/04

    logit.c:
    1) Added a new function logit_core()
    int logit_core( char *flag, char *format, va_list ap);
    This function is the same as logit(), except that it takes a va_list argument
    for the variable length parameter instead of '...', and it has an int
    return value.
    This function can be called by other functions that receive a '...' variable
    argument list, where as logit() cannot.  logit_core() is to logit()
    what vsprintf() is to sprintf().
    -
    2) Moved all of the functionality in logit() to logit_core(), and modify
    logit to call logit_core().
    -
    3)  Added a new function get_prog_name2(), as an intended replacement
    of get_prog_name().  get_prog_name2() includes an additional
    parameter (the buffer length of the output buffer).
    -
    4)  Modified logit_init() to use get_prog_name2() instead of get_prog_name()
    -
    All four(4) of these changes should be backwards compatible with all existing
    earthworm code, and the modified logit.c has already been tested with several
    earthworm modules.
    -

    ewdb_api:
    Added new function ewdb_api_GetEventSummaryInfo() to retrieve summary
    information for an event(including the preferred szSource and szSourceEventID
    of the event).   011904 DK

    KNOWN DEFICIENCIES:
    *******************
    k2ew: Kinemetrics control software has been modified to configure location
    codes inside the K2 itself (in previously unused space). k2ew has not yet
    been modified to read these location codes from the K2 header. For the
    time-being, location codes must be set with the "LocationNames" command
    in the config file.  Lynn Dietz 2007/02/09

    ringtocoax:
    In Windows NT, the time resolution of sleep_ew() is about 16 msec (one clock
    tick).  On Solaris, the resolution is about 10 msec.  This is a problem for
    ringtocoax, since packet delays need to be set to a few milliseconds.

    statmgr: A space is needed between "tsec:" and the value.
    If it isn't there, things fail. Artifcat of the kom routines. (Alex)

    threads functions: The KillThread function on WindowsNT and Solaris
    terminate the thread without ensuring that no mutexes are held. If a thread
    holds a mutex when it dies, no other thread can get that mutex. PNL 1/12/2000

    carlsubtrig:
    The system time must be set to GMT and ew_nt.cmd must have
    TZ=GMT for carlsubtrig to work.  Comments in ew_nt.cmd done 5/25/00. Barbara

    localmag:
    needs GMT set on the system

    ew2seisvole:
    on NT, exits with horrible crash when system is stopped.

    NUMBER OF RINGS LIMITED ON SOLARIS:
    Under Solaris 2.6 (and probably other versions as well), the maximum number
    of shared memory segments is six. This means that on an out-of-the-box machine
    you can only configure six rings. If you try to configure more than that, you
    will see a cryptic message from tport_create about too many open files.  The
    fix to this problem is to add the following lines to the /etc/system
    file, and then reboot the system.

    set shmsys:shminfo_shmmax = 4294967295
    set shmsys:shminfo_shmmin = 1
    set shmsys:shminfo_shmmni = 100
    set shmsys:shminfo_shmseg = 20
    set semsys:seminfo_semmns = 200
    set semsys:seminfo_semmni = 70

    This allows for 20 rings.

    Lucky Vidmar (7/6/2000)

    startstop_solaris:
    Fixed bug in call to logit_init().
    The program was printing error messages:
    Invalid arguments passed in.
    Call to get_prog_name failed.
    WARNING: Call logit_init before logit.

    startstop_solaris:
    There MAY be a problem with the signal that
    startstop sends to modules during the shutdown sequence. The shutdown
    sequence is started (after typing "quit" to startstop or running "pau")
    by startstop placing a terminate message on all transport rings. Modules
    should see this message and start their own shutdown. After a configurable
    delay, startstop checks to see that all modules have exitted. Any that are
    still running are sent a signal to terminate them. Currently that signal
    is SIG_TERM. But since wave_serverV has a handler for SIG_TERM, wave_serverV
    sees that as essentially the same as a terminate message. So if wave_serverV
    is having problems completing its shutdown, SIG_TERM won't do anything. The
    result is that startstop may give up and exit, leaving wave_serverV running.
    If that happens, the operator will have to terminate wave_serverV by doing
    "kill -9 ". That may leave shared memory and semaphores
    stranded in the kernel: run the command "ipcs -a" to see. If necessary,
    the stranded shared memory and semaphores may be cleaned up with the
    ipcrc command; must be run as root; see the man page.
    This problem only exists on Solaris/Unix, not on WindowsNT.
    PNL, 10/4/2000

    libsrc/utils/kom.c:  fix comment in k_open()

    The comment above k_open() says that only one file can
    be open at a time. Yet the Kbuf array has slots for MAXBUF (currently 4) open
    files. Does this work, or is the comment to be taken at it's word?
    PNL 10/15/00

    libsrc/utils/logit.c: logit_init() requires a module_id number, which it uses
    to construct the log file name. This is not helpful, since the module_id
    number is not meaningful to people. Worse, it requires that the config file be
    read and earthworm.d lookups be completed before logit calls can be made. Thus
    errors in the config file can only be reported to stderr or stdout instead of
    being saved in a file.  PNL 11/29/00

    libsrc/util/k2evt2ew.c: This library supports a maximum EVT data size
    of 800000 samples per channel per EVT file.  This value is hardcoded
    as MAXTRACELTH in include/k2evt2ew.h.  k2evt2ew() will return a warning
    if the EVT file exceeds this size, and process as much as the EVT file
    as the hardcoded limit allows.
    DK 2003/01/18

    import_ida:  Modified to build under WIN32(#ifdef'd a couple of includes
    and modified the NT makefiles.)  (saved under tag HYDRA_V1-20)
    Modified for SCNL and Tracebuf2.
    DK 2005/04/22

    TRACEBUF messages.
    The definition of `endtime' of the TRACEBUF message is not documented.
    Some programmers are taking it as the "expected start time of the next
    TRACEBUF packet (if the sample interval is uniform.)" The more accepted
    practice is that `endtime' is the time of the last sample of the current
    TRACEBUF packet; that is, one sample interval less than the expected
    start time of the next TRACEBUF messsage. Using this last definition, if a
    TRACEBUF packet has exactly one sample, then its starttime and endtime are
    the identical. Clearly this distinction needs to be documented. The file
    waveform_format (in the /home/earthworm/DOC directory) gives no specifics
    about start or end times.  PNL 1/24/01

### Download in other formats:

- Plain Text