#
ew2file Configuration File

(last revised May 15, 2010)

ew2file is a utility for writing out messages as a file (in binary form).

Below is a copy of the .d file with detailed notes on each parameter

    #   ew2file_generic configuration file
    #
    #
     MyModuleId     MOD_EW2FILE         # module id for this program
     InRing         SM_RING             # transport ring to use for input
     HeartBeatInt   30                  # EW internal heartbeat interval (sec)
     LogFile        1                   # If 0, don't write logfile
                                        # if 2, write to module log but not to
                                        # stderr/stdout .
    #
    # Logos of messages to export to client systems
    # Each message of a given logo will be written to a file with the specified
    # File Suffix at the end of the file name folloing `.'.
    # Do NOT include a `.' in the suffix.
    # Use as many GetMsgLogo commands as you want.
    #              Installation       Module       Message Type        File Suffix
     GetMsgLogo    INST_UCB        MOD_REDI2EW   TYPE_STRONGMOTIONII     smUCB

     MaxMsgSize        512         # maximum size (bytes) for input msgs
     QueueSize         1000        # number of msgs to buffer

     TimeBasedFilename 1           # set non-zero if you want a time string in the
                                   # form of "yyyymmdd-hhmmss." at the beginning of
                                   # each output file. The timestring is generated from
                                   # msg contents, currently possible for only msgtypes:
                                   # TYPE_PICK2K, TYPE_PICK_SCNL, TYPE_HYP2000ARC

    # OneFilePerMessage 1  		# an optional mode of ew2file to store all messages to a single file instead of
    				# the normal one file per message. This is useful for debugging purposes, or for gathering picks

    # Optional heartbeat file commands.
    #----------------------------------
    # Default HeartFileInt is 0 => send no heartbeat files.
    # Default HeartFileMsg is "Alive".
    # Default HeartFileSuffix is "hrt"
     HeartFileInt     30           # heartbeat file interval; optional
     HeartFileMsg     Alive        # string for heartbeat file; optional
     HeartFileSuffix  hrtUCB       # suffix for heartbeat files; do not include `.'

    # SerialKeeper: File name where the serial number of the output files is
    # stored. This should be a unique file name, in the params directory.
    # If the file does not exist, ew2file will attempt to create it.
    SerialKeeper  ew2file_keeper

    # TempDir: Directory in which files are created. This directory must be in the
    # same filesystem as all the SendDir directories. Exactly one TempDir is required.
    TempDir      /home/earthworm/run/ew2file/temp

    # SendDir: Directory to which output files will be moved after they have
    # been created.
    #  Use as many SendDir commands as you need.
    # Be sure the final line is terminated with a newline.
    SendDir      /home/earthworm/run/ew2file/Menlo
    SendDir	     /home/earthworm/run/ew2file/CGS
    SendDir	     /home/earthworm/run/ew2file/Pas

Module Index | ew2file Overview