    # The working copy of this file should live in the EW_PARAMS directory!!!

    #                       earthworm.d

    #              Earthworm administrative setup:
    #              Installation-specific info on
    #                    shared memory rings
    #                    module ids
    #                    message types

    #   Please read all comments before making changes to this file.
    #   The character string <-> numerical value mapping for certain
    #   module id's and message types are sacred to earthworm.d
    #   and must not be changed!!!

    #--------------------------------------------------------------------------
    #                      Shared Memory Ring Keys
    #
    # Define unique keys for shared memory regions (transport rings).
    # All string/value mappings for shared memory keys may be locally altered.
    #--------------------------------------------------------------------------

     Ring   WAVE_RING        1000    # public waveform data
     Ring   PICK_RING        1005    # public parametric data
     Ring   HYPO_RING        1015    # public hypocenters etc.
     Ring   BINDER_RING      1020    # private buffer for binder
     Ring   EQALARM_EW_RING  1025    # private buffer for eqalam_ew
     Ring   DRINK_RING       1030    # DST drink messages
     Ring   AD_RING          1035    # A/D waveform ring
     Ring   CUBIC_RING       1036    # private buffer for cubic_msg

    #--------------------------------------------------------------------------
    #                           Module IDs
    #
    #  Define all module name/module id pairs for this installation
    #  Except for MOD_WILDCARD, all string/value mappings for module ids
    #  may be locally altered. The character strings themselves may also
    #  be changed to be more meaningful for your installation.
    #
    #  0-255 are the only valid module ids.
    #--------------------------------------------------------------------------

     Module   MOD_WILDCARD        0   # Sacred wildcard value - DO NOT CHANGE!!!
     Module   MOD_ADSEND_A        1
     Module   MOD_ADSEND_B        2
     Module   MOD_ADSEND_C        3
     Module   MOD_PICKER_A        4
     Module   MOD_PICKER_B        5
     Module   MOD_PICK_EW         6
     Module   MOD_COAXTORING_A    7
     Module   MOD_COAXTORING_B    8
     Module   MOD_RINGTOCOAX      9
     Module   MOD_BINDER_EW      10
     Module   MOD_DISKMGR        11
     Module   MOD_STATMGR        14
     Module   MOD_REPORT         15
     Module   MOD_STARTSTOP      18
     Module   MOD_STATUS         19
     Module   MOD_NANOBOX        20
     Module   MOD_WAVESERVER     21
     Module   MOD_PAGERFEEDER    23
     Module   MOD_EQPROC         24
     Module   MOD_TANKPLAYER     25
     Module   MOD_EQALARM_EW     26
     Module   MOD_EQPRELIM       27
     Module   MOD_IMPORT_GENERIC 28
     Module   MOD_EXPORT_GENERIC 29
     Module   MOD_GETDST         31
     Module   MOD_LPTRIG_A       32
     Module   MOD_LPTRIG_B       33
     Module   MOD_TRG_ASSOC      34
     Module   MOD_AD_DEMUX_A     35
     Module   MOD_AD_DEMUX_B     36
     Module   MOD_VDL_EW         37
     Module   MOD_CUBIC_MSG      38
     Module   MOD_GAPLIST        39
     Module   MOD_GETTERW        40
     Module   MOD_WAVESERVERV    41
     Module   MOD_NANO2TRACE     42
     Module   MOD_GETDST2        43
     Module   MOD_EXPORT_SCN     44
     Module   MOD_ARC2TRIG       45
     Module   MOD_RCV_EW         48
     Module	  MOD_HELI1	     49

    #--------------------------------------------------------------------------
    #                          Message Types
    #
    #  Define all message name/message-type pairs for this installation.
    #  Valid numbers are:
    #
    #   0- 99 are reserved by "Earthworm Central" to label types of messages
    #         which may be exchanged between installations. These string/value
    #         mappings must be global to all Earthworm systems.
    #
    # 100-255 are controlled by each Earthworm installation. These values
    #         should be used to label messages which remain internal to
    #         an Earthworm system or installation. The character strings
    #         themselves should not be changed because the strings
    #         are often hard-coded into the modules. However, the
    #         string/value mappings can be locally altered.
    #--------------------------------------------------------------------------

    # Global (Sacred) Earthworm message-type mappings:
     Message  TYPE_WILDCARD        0  # Sacred wildcard value - DO NOT CHANGE!!!
     Message  TYPE_ADBUF           1  # multiplexed waveforms from DOS adsend
     Message  TYPE_ERROR           2  # error message
     Message  TYPE_HEARTBEAT       3  # heartbeat message
     Message  TYPE_NANOBUF         5  # single-channel waveforms from nanometrics
     Message  TYPE_PICK2K         10  # P-wave arrival time (with 4 digit year)
                                      #   from pick_ew
     Message  TYPE_CODA2K         11  # coda info (plus station code) from pick_ew
    #Message  TYPE_PICK2          12  # P-wave arrival time from picker & pick_ew
    #Message  TYPE_CODA2          13  # coda info from picker & pick_ew
     Message  TYPE_HYP2000ARC     14  # hyp2000 (Y2K hypoinverse) event archive
                                      #   msg from eqproc/eqprelim
     Message  TYPE_H71SUM2K       15  # hypo71-format hypocenter summary msg
                                      #   (with 4-digit year) from eqproc/eqprelim
    #Message  TYPE_HINVARC        17  # hypoinverse event archive msg from
                                      #   eqproc/eqprelim
    #Message  TYPE_H71SUM         18  # hypo71-format summary msg from
                                      #   eqproc/eqprelim
     Message  TYPE_TRACEBUF       20  # single-channel waveforms from NT adsend,
                                      #   getdst2, nano2trace, rcv_ew, import_ida...
     Message  TYPE_LPTRIG         21  # single-channel long-period trigger from
                                      #   lptrig & evanstrig
     Message  TYPE_CUBIC          22  # cubic-format summary msg from cubic_msg
     Message  TYPE_CARLSTATRIG    23  # single-channel trigger from carlstatrig
    #Message  TYPE_TRIGLIST       24  # trigger-list msg (used by tracesave modules)
                                      #   from arc2trig, trg_assoc, carlsubtrig
     Message  TYPE_TRIGLIST2K     25  # trigger-list msg (with 4-digit year) used
                                      #   by tracesave modules from arc2trig,
                                      #   trg_assoc, carlsubtrig
     Message  TYPE_TRACE_COMP_UA  26  # compressed waveforms from compress_UA

    # Installation-specific message-type mappings:
     Message  TYPE_SPECTRA       100
     Message  TYPE_QUAKE2K       101
     Message  TYPE_LINK          102
     Message  TYPE_EVENT2K       103
     Message  TYPE_PAGE          104
     Message  TYPE_KILL          105
     Message  TYPE_DSTDRINK      106
     Message  TYPE_RESTART       107
     Message  TYPE_REQSTATUS     108
     Message  TYPE_STATUS        109