# seisan_report Configuration File

(last revised April 23, 2015)

    # seisan_report parameter file

    #  Basic Earthworm setup:
    #
    MyModuleId         MOD_REPORT     # module id for this instance of report
    RingName           SSG_HYPO_RING  # ring to get input from
    HeartBeatInterval  60             # seconds between heartbeats
    LogFile            2              # 0 -> stdout, 1 -> stdout + file, 2 -> file
    Debug              1              # 0 for no diagnostics

    # Delay between detection of event and sfile being written (sec)
    # For wavefile to be in sfile this needs to be at least a few minutes
    WriteDelay         600

    # List the message logos to grab from transport ring
    #              Installation       Module          Message Types
    GetEventsFrom  INST_WILDCARD    MOD_WILDCARD      # hyp2000arc

    # Directory to write seisan files in
    SfileDir  ../../data/sausage_sfiles

    # Directory to find wav files
    WavDir ../../data/sausage_triggers

    # Agency for hypocentres and magnitudes. Note this can be a
    # maximum of 3 characters!! (Seisan requirement)
    Agency BGS

    # Switch to control whether alarm messages sent 0=no
    AlarmMsg  1

Module Index | seisan_report Overview