#
Ewthresh Configuration File

(last revised 28 April, 2011)

    #
    #         ewthresh Configuration File
    #
     MyModuleId     MOD_EWTHRESH     # module id for this program
     InRing         TEST_RING           # transport ring to use for input
     OutRing        HYPO_RING           # transport ring to use for output
     HeartBeatInt   30                  # EW internal heartbeat interval (sec)
     LogFile        1                   # If 0, don't write logfile; if 1, do
                                        # if 2, write to module log but not to
                                        # stderr/stdout
     MaxMsgSize     4096          # maximum size (bytes) for input/output msgs

     Threshold 0202 BHZ QT TT 749.0     # SCNL to monitor & threshold to look for

    # ThreshVotes NumTrig TimeSpanSeconds PreEventSeconds NumSCNLs SCNL1 SCNL2 ...
    # Generate a triglist message whenever NumTrig alarms occur within TimeSpanSecconds
    #    Time of message is PreEventSeconds before first trigger; listed SCNLs are included
    #
    # ThreshVotes 10 300 30 2 SSSS CCC NN LL ssss ccc nn ll

Module Index | Ewthresh Overview